#!/bin/sh
#
# Copyright (C) 2010 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/cns21xx.sh

board=$(get_board_name)

case "$board" in
"ns-k330")
	ucidef_set_led_netdev "eth_orange" "ETH (orange)" "ns-k330:orange:eth" "eth0"
	ucidef_set_led_usbdev "usb1" "USB1" "ns-k330:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "ns-k330:green:usb2" "1-2"
	;;
fi

ucidef_commit_leds

exit 0
