--- a/arch/powerpc/boot/dts/mpc8548cds.dts
+++ b/arch/powerpc/boot/dts/mpc8548cds.dts
@@ -260,8 +260,10 @@
 					#address-cells = <0>;
 					#interrupt-cells = <2>;
 					compatible = "chrp,iic";
+/*
 					interrupts = <0 1 0 0>;
 					interrupt-parent = <&mpic>;
+*/
 				};
 
 				rtc@70 {
