--- a/arch/arm/mach-ixp4xx/avila-setup.c
+++ b/arch/arm/mach-ixp4xx/avila-setup.c
@@ -14,9 +14,16 @@
 #include <linux/kernel.h>
 #include <linux/init.h>
 #include <linux/device.h>
+#include <linux/if_ether.h>
+#include <linux/socket.h>
+#include <linux/netdevice.h>
 #include <linux/serial.h>
 #include <linux/tty.h>
 #include <linux/serial_8250.h>
+#include <linux/i2c.h>
+#include <linux/i2c/at24.h>
+#include <linux/leds.h>
+#include <linux/i2c/pca953x.h>
 #include <linux/i2c-gpio.h>
 #include <asm/types.h>
 #include <asm/setup.h>
@@ -26,10 +33,25 @@
 #include <asm/irq.h>
 #include <asm/mach/arch.h>
 #include <asm/mach/flash.h>
+#include <linux/irq.h>
 
 #define AVILA_SDA_PIN	7
 #define AVILA_SCL_PIN	6
 
+/* User LEDs */
+#define AVILA_GW23XX_LED_USER_GPIO     3
+#define AVILA_GW23X7_LED_USER_GPIO     4
+
+/* gpio mask used by platform device */
+#define AVILA_GPIO_MASK        (1 << 1) | (1 << 3) | (1 << 5) | (1 << 7) | (1 << 9)
+
+struct avila_board_info {
+	unsigned char	*model;
+	void		(*setup)(void);
+};
+
+static struct avila_board_info *avila_info __initdata;
+
 static struct flash_platform_data avila_flash_data = {
 	.map_name	= "cfi_probe",
 	.width		= 2,
@@ -105,14 +127,69 @@ static struct platform_device avila_uart
 	.resource		= avila_uart_resources
 };
 
-static struct resource avila_pata_resources[] = {
+static struct resource avila_optional_uart_resources[] = {
 	{
-		.flags	= IORESOURCE_MEM
-	},
+		.start  = 0x54000000,
+		.end  = 0x54000fff,
+		.flags  = IORESOURCE_MEM
+	},{
+		.start  = 0x55000000,
+		.end  = 0x55000fff,
+		.flags  = IORESOURCE_MEM
+	},{
+		.start  = 0x56000000,
+		.end  = 0x56000fff,
+		.flags  = IORESOURCE_MEM
+	},{
+		.start  = 0x57000000,
+		.end  = 0x57000fff,
+		.flags  = IORESOURCE_MEM
+	}
+};
+
+static struct plat_serial8250_port avila_optional_uart_data[] = {
 	{
-		.flags	= IORESOURCE_MEM,
+		.flags    = UPF_BOOT_AUTOCONF,
+		.iotype   = UPIO_MEM,
+		.regshift = 0,
+		.uartclk  = 18432000,
+		.rw_delay = 2,
+	},{
+		.flags    = UPF_BOOT_AUTOCONF,
+		.iotype   = UPIO_MEM,
+		.regshift = 0,
+		.uartclk  = 18432000,
+		.rw_delay = 2,
+	},{
+		.flags    = UPF_BOOT_AUTOCONF,
+		.iotype   = UPIO_MEM,
+		.regshift = 0,
+		.uartclk  = 18432000,
+		.rw_delay = 2,
+	},{
+		.flags    = UPF_BOOT_AUTOCONF,
+		.iotype   = UPIO_MEM,
+		.regshift = 0,
+		.uartclk  = 18432000,
+		.rw_delay = 2,
 	},
+	{ }
+};
+
+static struct platform_device avila_optional_uart = {
+  .name   = "serial8250",
+  .id   = PLAT8250_DEV_PLATFORM1,
+  .dev.platform_data  = avila_optional_uart_data,
+  .num_resources  = 4,
+  .resource = avila_optional_uart_resources,
+};
+
+static struct resource avila_pata_resources[] = {
 	{
+		.flags	= IORESOURCE_MEM
+	},{
+		.flags	= IORESOURCE_MEM,
+	},{
 		.name	= "intrq",
 		.start	= IRQ_IXP4XX_GPIO12,
 		.end	= IRQ_IXP4XX_GPIO12,
@@ -133,21 +210,280 @@ static struct platform_device avila_pata
 	.resource		= avila_pata_resources,
 };
 
+/* Built-in 10/100 Ethernet MAC interfaces */
+static struct eth_plat_info avila_npeb_data = {
+	.phy		= 0,
+	.rxq		= 3,
+	.txreadyq	= 20,
+};
+
+static struct eth_plat_info avila_npec_data = {
+	.phy		= 1,
+	.rxq		= 4,
+	.txreadyq	= 21,
+};
+
+static struct platform_device avila_npeb_device = {
+	.name			= "ixp4xx_eth",
+	.id			= IXP4XX_ETH_NPEB,
+	.dev.platform_data	= &avila_npeb_data,
+};
+
+static struct platform_device avila_npec_device = {
+	.name			= "ixp4xx_eth",
+	.id			= IXP4XX_ETH_NPEC,
+	.dev.platform_data	= &avila_npec_data,
+};
+
+static struct gpio_led avila_gpio_leds[] = {
+	{
+		.name		= "user",  /* green led */
+		.gpio		= AVILA_GW23XX_LED_USER_GPIO,
+		.active_low	= 1,
+	},
+	{
+		.name		= "radio1",  /* green led */
+		.gpio		= 104,
+		.active_low	= 1,
+	},
+	{
+		.name		= "radio2",  /* green led */
+		.gpio		= 105,
+		.active_low	= 1,
+	},
+	{
+		.name		= "radio3",  /* green led */
+		.gpio		= 106,
+		.active_low	= 1,
+	},
+	{
+		.name		= "radio4",  /* green led */
+		.gpio		= 107,
+		.active_low	= 1,
+	},
+
+};
+
+static struct gpio_led_platform_data avila_gpio_leds_data = {
+	.num_leds		= 1,
+	.leds			= avila_gpio_leds,
+};
+
+static struct platform_device avila_gpio_leds_device = {
+	.name			= "leds-gpio",
+	.id			= -1,
+	.dev.platform_data	= &avila_gpio_leds_data,
+};
+
+static struct latch_led avila_latch_leds[] = {
+	{
+		.name	= "led0",  /* green led */
+		.bit	= 0,
+	},
+	{
+		.name	= "led1",  /* green led */
+		.bit	= 1,
+	},
+	{
+		.name	= "led2",  /* green led */
+		.bit	= 2,
+	},
+	{
+		.name	= "led3",  /* green led */
+		.bit	= 3,
+	},
+	{
+		.name	= "led4",  /* green led */
+		.bit	= 4,
+	},
+	{
+		.name	= "led5",  /* green led */
+		.bit	= 5,
+	},
+	{
+		.name	= "led6",  /* green led */
+		.bit	= 6,
+	},
+	{
+		.name	= "led7",  /* green led */
+		.bit	= 7,
+	}
+};
+
+static struct latch_led_platform_data avila_latch_leds_data = {
+	.num_leds	= 8,
+	.leds		= avila_latch_leds,
+	.mem		= 0x51000000,
+};
+
+static struct platform_device avila_latch_leds_device = {
+	.name			= "leds-latch",
+	.id			= -1,
+	.dev.platform_data	= &avila_latch_leds_data,
+};
+
 static struct platform_device *avila_devices[] __initdata = {
 	&avila_i2c_gpio,
-	&avila_flash,
 	&avila_uart
 };
 
-static void __init avila_init(void)
+static struct platform_device avila_gpio_dev = {
+	.name     = "GPIODEV",
+	.id     = -1,
+};
+
+/*
+ * Audio Devices
+ */
+
+static struct platform_device avila_hss_device[] = {
+	{
+		.name = "gw_avila_hss",
+		.id = 0,
+	},{
+		.name = "gw_avila_hss",
+		.id = 1,
+	},{
+		.name = "gw_avila_hss",
+		.id = 2,
+	},{
+		.name = "gw_avila_hss",
+		.id = 3,
+	},
+};
+
+static struct platform_device avila_pcm_device[] = {
+	{
+		.name = "gw_avila-audio",
+		.id = 0,
+	},{
+		.name = "gw_avila-audio",
+		.id = 1,
+	},{
+		.name = "gw_avila-audio",
+		.id = 2,
+	},{
+		.name = "gw_avila-audio",
+		.id = 3,
+	}
+};
+
+static void setup_audio_devices(void) {
+	platform_device_register(&avila_hss_device[0]);
+	platform_device_register(&avila_hss_device[1]);
+	platform_device_register(&avila_hss_device[2]);
+	platform_device_register(&avila_hss_device[3]);
+
+	platform_device_register(&avila_pcm_device[0]);
+	platform_device_register(&avila_pcm_device[1]);
+	platform_device_register(&avila_pcm_device[2]);
+	platform_device_register(&avila_pcm_device[3]);
+}
+
+static void __init avila_gw23xx_setup(void)
 {
-	ixp4xx_sys_init();
+	platform_device_register(&avila_npeb_device);
+	platform_device_register(&avila_npec_device);
 
-	avila_flash_resource.start = IXP4XX_EXP_BUS_BASE(0);
-	avila_flash_resource.end =
-		IXP4XX_EXP_BUS_BASE(0) + ixp4xx_exp_bus_size - 1;
+	platform_device_register(&avila_gpio_leds_device);
+}
 
-	platform_add_devices(avila_devices, ARRAY_SIZE(avila_devices));
+static void __init avila_gw2342_setup(void)
+{
+	platform_device_register(&avila_npeb_device);
+	platform_device_register(&avila_npec_device);
+
+	platform_device_register(&avila_gpio_leds_device);
+
+	avila_pata_resources[0].start = IXP4XX_EXP_BUS_BASE(1);
+	avila_pata_resources[0].end = IXP4XX_EXP_BUS_END(1);
+
+	avila_pata_resources[1].start = IXP4XX_EXP_BUS_BASE(2);
+	avila_pata_resources[1].end = IXP4XX_EXP_BUS_END(2);
+
+	avila_pata_data.cs0_cfg = IXP4XX_EXP_CS1;
+	avila_pata_data.cs1_cfg = IXP4XX_EXP_CS2;
+
+	platform_device_register(&avila_pata);
+}
+
+static void __init avila_gw2345_setup(void)
+{
+	avila_npeb_data.phy = IXP4XX_ETH_PHY_MAX_ADDR;
+	avila_npeb_data.phy_mask = 0x1e; /* ports 1-4 of the KS8995 switch */
+	platform_device_register(&avila_npeb_device);
+
+	avila_npec_data.phy = 5; /* port 5 of the KS8995 switch */
+	platform_device_register(&avila_npec_device);
+
+	platform_device_register(&avila_gpio_leds_device);
+
+	avila_pata_resources[0].start = IXP4XX_EXP_BUS_BASE(1);
+	avila_pata_resources[0].end = IXP4XX_EXP_BUS_END(1);
+
+	avila_pata_resources[1].start = IXP4XX_EXP_BUS_BASE(2);
+	avila_pata_resources[1].end = IXP4XX_EXP_BUS_END(2);
+
+	avila_pata_data.cs0_cfg = IXP4XX_EXP_CS1;
+	avila_pata_data.cs1_cfg = IXP4XX_EXP_CS2;
+
+	platform_device_register(&avila_pata);
+}
+
+static void __init avila_gw2347_setup(void)
+{
+	platform_device_register(&avila_npeb_device);
+
+	avila_gpio_leds[0].gpio = AVILA_GW23X7_LED_USER_GPIO;
+	platform_device_register(&avila_gpio_leds_device);
+}
+
+static void __init avila_gw2348_setup(void)
+{
+	platform_device_register(&avila_npeb_device);
+	platform_device_register(&avila_npec_device);
+
+	platform_device_register(&avila_gpio_leds_device);
+
+	avila_pata_resources[0].start = IXP4XX_EXP_BUS_BASE(1);
+	avila_pata_resources[0].end = IXP4XX_EXP_BUS_END(1);
+
+	avila_pata_resources[1].start = IXP4XX_EXP_BUS_BASE(2);
+	avila_pata_resources[1].end = IXP4XX_EXP_BUS_END(2);
+
+	avila_pata_data.cs0_cfg = IXP4XX_EXP_CS1;
+	avila_pata_data.cs1_cfg = IXP4XX_EXP_CS2;
+
+	platform_device_register(&avila_pata);
+}
+
+static void __init avila_gw2353_setup(void)
+{
+	platform_device_register(&avila_npeb_device);
+	platform_device_register(&avila_gpio_leds_device);
+}
+
+static void __init avila_gw2355_setup(void)
+{
+	avila_npeb_data.phy = IXP4XX_ETH_PHY_MAX_ADDR;
+	avila_npeb_data.phy_mask = 0x1e; /* ports 1-4 of the KS8995 switch */
+	platform_device_register(&avila_npeb_device);
+
+	avila_npec_data.phy = 16;
+	platform_device_register(&avila_npec_device);
+
+	avila_gpio_leds[0].gpio = AVILA_GW23X7_LED_USER_GPIO;
+	platform_device_register(&avila_gpio_leds_device);
+
+	*IXP4XX_EXP_CS4 |= 0xbfff3c03;
+	avila_latch_leds[0].name = "RXD";
+	avila_latch_leds[1].name = "TXD";
+	avila_latch_leds[2].name = "POL";
+	avila_latch_leds[3].name = "LNK";
+	avila_latch_leds[4].name = "ERR";
+	avila_latch_leds_data.num_leds = 5;
+	avila_latch_leds_data.mem = 0x54000000;
+	platform_device_register(&avila_latch_leds_device);
 
 	avila_pata_resources[0].start = IXP4XX_EXP_BUS_BASE(1);
 	avila_pata_resources[0].end = IXP4XX_EXP_BUS_END(1);
@@ -159,8 +495,274 @@ static void __init avila_init(void)
 	avila_pata_data.cs1_cfg = IXP4XX_EXP_CS2;
 
 	platform_device_register(&avila_pata);
+}
+
+static void __init avila_gw2357_setup(void)
+{
+	platform_device_register(&avila_npeb_device);
+
+	avila_gpio_leds[0].gpio = AVILA_GW23X7_LED_USER_GPIO;
+	platform_device_register(&avila_gpio_leds_device);
+
+	*IXP4XX_EXP_CS1 |= 0xbfff3c03;
+	platform_device_register(&avila_latch_leds_device);
+}
+
+static void __init avila_gw2365_setup(void)
+{
+	avila_flash_resource.end = IXP4XX_EXP_BUS_BASE(0) + SZ_32M - 1;
+
+	*IXP4XX_EXP_CS4 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO0, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[0].mapbase = 0x54000000;
+	avila_optional_uart_data[0].membase = (void __iomem *)ioremap(0x54000000, 0x0fff);
+	avila_optional_uart_data[0].irq   = IRQ_IXP4XX_GPIO0;
+
+	*IXP4XX_EXP_CS5 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO1, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[1].mapbase = 0x55000000;
+	avila_optional_uart_data[1].membase = (void __iomem *)ioremap(0x55000000, 0x0fff);
+	avila_optional_uart_data[1].irq   = IRQ_IXP4XX_GPIO1;
+
+	*IXP4XX_EXP_CS6 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO2, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[2].mapbase = 0x56000000;
+	avila_optional_uart_data[2].membase = (void __iomem *)ioremap(0x56000000, 0x0fff);
+	avila_optional_uart_data[2].irq   = IRQ_IXP4XX_GPIO2;
+
+	*IXP4XX_EXP_CS7 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO3, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[3].mapbase = 0x57000000;
+	avila_optional_uart_data[3].membase = (void __iomem *)ioremap(0x57000000, 0x0fff);
+	avila_optional_uart_data[3].irq   = IRQ_IXP4XX_GPIO3;
+
+	platform_device_register(&avila_optional_uart);
+
+	avila_npeb_data.phy = 1;
+	platform_device_register(&avila_npeb_device);
+
+	avila_npec_data.phy = 2;
+	platform_device_register(&avila_npec_device);
+
+	avila_pata_resources[0].start = IXP4XX_EXP_BUS_BASE(2);
+	avila_pata_resources[0].end = IXP4XX_EXP_BUS_END(2);
+
+	avila_pata_resources[1].start = IXP4XX_EXP_BUS_BASE(3);
+	avila_pata_resources[1].end = IXP4XX_EXP_BUS_END(3);
+
+	avila_pata_data.cs0_cfg = IXP4XX_EXP_CS2;
+	avila_pata_data.cs1_cfg = IXP4XX_EXP_CS3;
+
+	platform_device_register(&avila_pata);
+
+	avila_gpio_leds[0].gpio = 109;
+	avila_gpio_leds_data.num_leds = 5;
+	platform_device_register(&avila_gpio_leds_device);
+
+	setup_audio_devices();
+}
+
+static void __init avila_gw2369_setup(void)
+{
+	avila_flash_resource.end = IXP4XX_EXP_BUS_BASE(0) + SZ_32M - 1;
+
+	avila_npeb_data.phy = 1;
+	platform_device_register(&avila_npeb_device);
+
+	avila_npec_data.phy = 2;
+	platform_device_register(&avila_npec_device);
+
+	setup_audio_devices();
+}
+
+static void __init avila_gw2370_setup(void)
+{
+	avila_flash_resource.end = IXP4XX_EXP_BUS_BASE(0) + SZ_32M - 1;
+
+	avila_npeb_data.phy = 5;
+	platform_device_register(&avila_npeb_device);
+
+	avila_npec_data.phy = IXP4XX_ETH_PHY_MAX_ADDR;
+	avila_npec_data.phy_mask = 0x1e; /* ports 1-4 of the KS8995 switch */
+	platform_device_register(&avila_npec_device);
+
+	*IXP4XX_EXP_CS2 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO2, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[0].mapbase = 0x52000000;
+	avila_optional_uart_data[0].membase = (void __iomem *)ioremap(0x52000000, 0x0fff);
+	avila_optional_uart_data[0].irq   = IRQ_IXP4XX_GPIO2;
+
+	*IXP4XX_EXP_CS3 = 0xBFFF3C43;
+	irq_set_irq_type(IRQ_IXP4XX_GPIO3, IRQ_TYPE_EDGE_RISING);
+	avila_optional_uart_data[1].mapbase = 0x53000000;
+	avila_optional_uart_data[1].membase = (void __iomem *)ioremap(0x53000000, 0x0fff);
+	avila_optional_uart_data[1].irq   = IRQ_IXP4XX_GPIO3;
+
+	avila_optional_uart.num_resources = 2;
+
+	platform_device_register(&avila_optional_uart);
+
+	avila_gpio_leds[0].gpio = 101;
+	platform_device_register(&avila_gpio_leds_device);
+
+	setup_audio_devices();
+}
+
+
+
+static struct avila_board_info avila_boards[] __initdata = {
+	{
+		.model		= "GW2342",
+		.setup		= avila_gw2342_setup,
+	}, {
+		.model		= "GW2345",
+		.setup		= avila_gw2345_setup,
+	}, {
+		.model		= "GW2347",
+		.setup		= avila_gw2347_setup,
+	}, {
+		.model		= "GW2348",
+		.setup		= avila_gw2348_setup,
+	}, {
+		.model		= "GW2353",
+		.setup		= avila_gw2353_setup,
+	}, {
+		.model		= "GW2355",
+		.setup		= avila_gw2355_setup,
+	}, {
+		.model		= "GW2357",
+		.setup		= avila_gw2357_setup,
+	}, {
+		.model		= "GW2365",
+		.setup		= avila_gw2365_setup,
+	}, {
+		.model		= "GW2369",
+		.setup		= avila_gw2369_setup,
+	}, {
+		.model		= "GW2370",
+		.setup		= avila_gw2370_setup,
+	}, {
+		.model		= "GW2373",
+		.setup		= avila_gw2369_setup,
+	}
+};
+
+static struct avila_board_info * __init avila_find_board_info(char *model)
+{
+	int i;
+	model[6] = '\0';
+
+	for (i = 0; i < ARRAY_SIZE(avila_boards); i++) {
+		struct avila_board_info *info = &avila_boards[i];
+		if (strcmp(info->model, model) == 0)
+			return info;
+	}
+
+	return NULL;
+}
+
+static struct memory_accessor *at24_mem_acc;
+
+static void at24_setup(struct memory_accessor *mem_acc, void *context)
+{
+	char mac_addr[ETH_ALEN];
+	char model[7];
+
+	at24_mem_acc = mem_acc;
+
+	/* Read MAC addresses */
+	if (at24_mem_acc->read(at24_mem_acc, mac_addr, 0x0, 6) == 6) {
+		memcpy(&avila_npeb_data.hwaddr, mac_addr, ETH_ALEN);
+	}
+	if (at24_mem_acc->read(at24_mem_acc, mac_addr, 0x6, 6) == 6) {
+		memcpy(&avila_npec_data.hwaddr, mac_addr, ETH_ALEN);
+	}
+
+	/* Read the first 6 bytes of the model number */
+	if (at24_mem_acc->read(at24_mem_acc, model, 0x20, 6) == 6) {
+		avila_info = avila_find_board_info(model);
+	}
+
+}
+
+static struct at24_platform_data avila_eeprom_info = {
+	.byte_len	= 1024,
+	.page_size	= 16,
+//	.flags		= AT24_FLAG_READONLY,
+	.setup		= at24_setup,
+};
+
+static struct pca953x_platform_data avila_pca_data = {
+	.gpio_base  = 100,
+};
+
+static struct i2c_board_info __initdata avila_i2c_board_info[] = {
+	{
+		I2C_BOARD_INFO("ds1672", 0x68),
+	},
+	{
+		I2C_BOARD_INFO("gsp", 0x29),
+	},
+	{
+		I2C_BOARD_INFO("pca9555", 0x23),
+		.platform_data = &avila_pca_data,
+	},
+	{
+		I2C_BOARD_INFO("ad7418", 0x28),
+	},
+	{
+		I2C_BOARD_INFO("24c08", 0x51),
+		.platform_data	= &avila_eeprom_info
+	},
+	{
+		I2C_BOARD_INFO("tlv320aic33", 0x1b),
+	},
+	{
+		I2C_BOARD_INFO("tlv320aic33", 0x1a),
+	},
+	{
+		I2C_BOARD_INFO("tlv320aic33", 0x19),
+	},
+	{
+		I2C_BOARD_INFO("tlv320aic33", 0x18),
+	},
+};
+
+static void __init avila_init(void)
+{
+	ixp4xx_sys_init();
+
+	platform_add_devices(avila_devices, ARRAY_SIZE(avila_devices));
+
+	i2c_register_board_info(0, avila_i2c_board_info,
+			ARRAY_SIZE(avila_i2c_board_info));
+
+	platform_device_register(&avila_gpio_dev);
+}
+
+static int __init avila_model_setup(void)
+{
+	if (!machine_is_avila())
+		return 0;
+
+	/* default 16MB flash */
+	avila_flash_resource.start = IXP4XX_EXP_BUS_BASE(0);
+	avila_flash_resource.end = IXP4XX_EXP_BUS_BASE(0) + SZ_16M - 1;
+
+	if (avila_info) {
+		printk(KERN_DEBUG "Running on Gateworks Avila %s\n",
+							avila_info->model);
+		avila_info->setup();
+	} else {
+		printk(KERN_INFO "Unknown/missing Avila model number"
+						" -- defaults will be used\n");
+		avila_gw23xx_setup();
+	}
+	platform_device_register(&avila_flash);
 
+	return 0;
 }
+late_initcall(avila_model_setup);
 
 MACHINE_START(AVILA, "Gateworks Avila Network Platform")
 	/* Maintainer: Deepak Saxena <dsaxena@plexity.net> */
--- a/arch/arm/mach-ixp4xx/avila-pci.c
+++ b/arch/arm/mach-ixp4xx/avila-pci.c
@@ -27,8 +27,8 @@
 #include <mach/hardware.h>
 #include <asm/mach-types.h>
 
-#define AVILA_MAX_DEV	4
-#define LOFT_MAX_DEV	6
+#define AVILA_MAX_DEV	6
+
 #define IRQ_LINES	4
 
 /* PCI controller GPIO to IRQ pin mappings */
@@ -55,9 +55,7 @@ static int __init avila_map_irq(const st
 		IXP4XX_GPIO_IRQ(INTD)
 	};
 
-	if (slot >= 1 &&
-	    slot <= (machine_is_loft() ? LOFT_MAX_DEV : AVILA_MAX_DEV) &&
-	    pin >= 1 && pin <= IRQ_LINES)
+	if (slot >= 1 && slot <= AVILA_MAX_DEV && pin >= 1 && pin <= IRQ_LINES)
 		return pci_irq_table[(slot + pin - 2) % 4];
 
 	return -1;
