--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -376,7 +376,7 @@ static void __devinit ssb_pcicore_init_h
 	set_io_port_base(ssb_pcicore_controller.io_map_base);
 	/* Give some time to the PCI controller to configure itself with the new
 	 * values. Not waiting at this point causes crashes of the machine. */
-	mdelay(10);
+	mdelay(300);
 	register_pci_controller(&ssb_pcicore_controller);
 }
 
