--- a/arch/mips/bcm47xx/setup.c
+++ b/arch/mips/bcm47xx/setup.c
@@ -190,6 +190,8 @@ static void __init bcm47xx_register_bcma
 	err = bcma_host_soc_register(&bcm47xx_bus.bcma);
 	if (err)
 		panic("Failed to initialize BCMA bus (err %d)", err);
+
+	bcm47xx_fill_bcma_boardinfo(&bcm47xx_bus.bcma.bus.boardinfo, NULL);
 }
 #endif
 
--- a/arch/mips/bcm47xx/sprom.c
+++ b/arch/mips/bcm47xx/sprom.c
@@ -630,3 +630,15 @@ void bcm47xx_fill_ssb_boardinfo(struct s
 	nvram_read_u16(prefix, NULL, "boardtype", &boardinfo->type, 0);
 }
 #endif
+
+#ifdef CONFIG_BCM47XX_BCMA
+void bcm47xx_fill_bcma_boardinfo(struct bcma_boardinfo *boardinfo,
+				 const char *prefix)
+{
+	nvram_read_u16(prefix, NULL, "boardvendor", &boardinfo->vendor, 0);
+	if (!boardinfo->vendor)
+		boardinfo->vendor = SSB_BOARDVENDOR_BCM;
+
+	nvram_read_u16(prefix, NULL, "boardtype", &boardinfo->type, 0);
+}
+#endif
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
@@ -51,5 +51,9 @@ void bcm47xx_fill_sprom_ethernet(struct
 void bcm47xx_fill_ssb_boardinfo(struct ssb_boardinfo *boardinfo,
 				const char *prefix);
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+void bcm47xx_fill_bcma_boardinfo(struct bcma_boardinfo *boardinfo,
+				 const char *prefix);
+#endif
 
 #endif /* __ASM_BCM47XX_H */
