--- a/arch/arm/Kconfig
+++ b/arch/arm/Kconfig
@@ -1104,10 +1104,15 @@ source "arch/arm/mach-vt8500/Kconfig"
 
 source "arch/arm/mach-w90x900/Kconfig"
 
+source "arch/arm/plat-fa/Kconfig"
+
 # Definitions to make life easier
 config ARCH_ACORN
 	bool
 
+config PLAT_FA
+	bool
+
 config PLAT_IOP
 	bool
 	select GENERIC_CLOCKEVENTS
--- a/arch/arm/Makefile
+++ b/arch/arm/Makefile
@@ -203,6 +203,7 @@ plat-$(CONFIG_ARCH_MXC)		:= mxc
 plat-$(CONFIG_ARCH_OMAP)	:= omap
 plat-$(CONFIG_ARCH_S3C64XX)	:= samsung
 plat-$(CONFIG_ARCH_ZYNQ)	:= versatile
+plat-$(CONFIG_PLAT_FA)		:= fa
 plat-$(CONFIG_PLAT_IOP)		:= iop
 plat-$(CONFIG_PLAT_NOMADIK)	:= nomadik
 plat-$(CONFIG_PLAT_ORION)	:= orion
@@ -301,7 +302,7 @@ define archhelp
   echo  '  Image         - Uncompressed kernel image (arch/$(ARCH)/boot/Image)'
   echo  '* xipImage      - XIP kernel image, if configured (arch/$(ARCH)/boot/xipImage)'
   echo  '  uImage        - U-Boot wrapped zImage'
-  echo  '  bootpImage    - Combined zImage and initial RAM disk' 
+  echo  '  bootpImage    - Combined zImage and initial RAM disk'
   echo  '                  (supply initrd image via make variable INITRD=<path>)'
   echo  '  dtbs          - Build device tree blobs for enabled boards'
   echo  '  install       - Install uncompressed kernel'
--- /dev/null
+++ b/arch/arm/plat-fa/Makefile
@@ -0,0 +1,10 @@
+#
+# Makefile for the linux kernel.
+#
+
+obj-y :=
+
+obj-m :=
+obj-n :=
+obj-  :=
+
--- /dev/null
+++ b/arch/arm/plat-fa/Kconfig
@@ -0,0 +1,3 @@
+if PLAT_FA
+
+endif
