From f0649f7b7c672cf452a1796a1422bf615e1973f8 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Tue, 29 May 2012 11:01:12 +0200
Subject: [PATCH] MIPS: BCM63XX: add 963281TAN reference board

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |   71 +++++++++++++++++++++++++++++
 1 files changed, 71 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -125,6 +125,76 @@ static struct board_info __initdata boar
 		},
 	},
 };
+
+static struct board_info __initdata board_963281TAN = {
+	.name				= "963281TAN",
+	.expected_cpu_id		= 0x6328,
+
+	.has_uart0			= 1,
+	.has_pci			= 1,
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[0] = {
+				.used	= 1,
+				.phy_id = 1,
+				.name	= "Port 1",
+			},
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "Port 2",
+			},
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "Port 3",
+			},
+			[3] = {
+				.used	= 1,
+				.phy_id	= 4,
+				.name	= "Port 4",
+			},
+		},
+	},
+
+	.leds = {
+		{
+			.name		= "963281TAN::internet",
+			.gpio		= 1,
+			.active_low	= 1,
+		},
+		{
+			.name		= "963281TAN::power",
+			.gpio		= 4,
+			.active_low	= 1,
+			.default_trigger = "default-on",
+		},
+		{
+			.name		= "963281TAN::internet-fail",
+			.gpio		= 7,
+			.active_low	= 1,
+		},
+		{
+			.name		= "963281TAN::power-fail",
+			.gpio		= 8,
+			.active_low	= 1,
+		},
+		{
+			.name		= "963281TAN::wps",
+			.gpio		= 9,
+			.active_low	= 1,
+		},
+		{
+			.name		= "963281TAN::dsl",
+			.gpio		= 11,
+			.active_low	= 1,
+		},
+
+	},
+};
 #endif
 
 /*
@@ -2322,6 +2392,7 @@ static struct board_info __initdata boar
 static const struct board_info __initdata *bcm963xx_boards[] = {
 #ifdef CONFIG_BCM63XX_CPU_6328
 	&board_96328avng,
+	&board_963281TAN,
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6338
 	&board_96338gw,
