From 27ebbb819b1f92d52309276b29b7a56e362e5c4d Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Mon, 21 Nov 2011 00:48:52 +0100
Subject: [PATCH 54/84] MIPS: BCM63XX: add basic BCM6362 support

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 arch/mips/bcm63xx/Kconfig                         |    4 +
 arch/mips/bcm63xx/boards/board_bcm963xx.c         |    2 +-
 arch/mips/bcm63xx/cpu.c                           |   52 ++++++++-
 arch/mips/bcm63xx/irq.c                           |   19 +++
 arch/mips/bcm63xx/prom.c                          |    2 +
 arch/mips/bcm63xx/setup.c                         |    3 +
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h  |  139 +++++++++++++++++++++
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h |    2 +
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h |   59 +++++++++
 arch/mips/include/asm/mach-bcm63xx/ioremap.h      |    1 +
 10 files changed, 281 insertions(+), 2 deletions(-)

--- a/arch/mips/bcm63xx/Kconfig
+++ b/arch/mips/bcm63xx/Kconfig
@@ -25,6 +25,10 @@ config BCM63XX_CPU_6358
 	bool "support 6358 CPU"
 	select HW_HAS_PCI
 
+config BCM63XX_CPU_6362
+	bool "support 6362 CPU"
+	select HW_HAS_PCI
+
 config BCM63XX_CPU_6368
 	bool "support 6368 CPU"
 	select HW_HAS_PCI
--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -764,7 +764,7 @@ void __init board_prom_init(void)
 	/* read base address of boot chip select (0)
 	 * 6328 does not have MPI but boots from a fixed address
 	 */
-	if (BCMCPU_IS_6328())
+	if (BCMCPU_IS_6328() || BCMCPU_IS_6362())
 		val = 0x18000000;
 	else {
 		val = bcm_mpi_readl(MPI_CSBASE_REG(0));
--- a/arch/mips/bcm63xx/cpu.c
+++ b/arch/mips/bcm63xx/cpu.c
@@ -71,6 +71,15 @@ static const int bcm6358_irqs[] = {
 
 };
 
+static const unsigned long bcm6362_regs_base[] = {
+	__GEN_CPU_REGS_TABLE(6362)
+};
+
+static const int bcm6362_irqs[] = {
+	__GEN_CPU_IRQ_TABLE(6362)
+
+};
+
 static const unsigned long bcm6368_regs_base[] = {
 	__GEN_CPU_REGS_TABLE(6368)
 };
@@ -169,6 +178,42 @@ static unsigned int detect_cpu_clock(voi
 		return (16 * 1000000 * n1 * n2) / m1;
 	}
 
+	case BCM6362_CPU_ID:
+	{
+		unsigned int tmp, mips_pll_fcvo;
+
+		tmp = bcm_misc_readl(MISC_STRAPBUS_6362_REG);
+		mips_pll_fcvo = (tmp & STRAPBUS_6362_FCVO_MASK)
+				>> STRAPBUS_6362_FCVO_SHIFT;
+		switch (mips_pll_fcvo) {
+		case 0x03:
+		case 0x0b:
+		case 0x13:
+		case 0x1b:
+			return 240000000;
+		case 0x04:
+		case 0x0c:
+		case 0x14:
+		case 0x1c:
+			return 160000000;
+		case 0x05:
+		case 0x0e:
+		case 0x16:
+		case 0x1e:
+		case 0x1f:
+			return 400000000;
+		case 0x06:
+			return 440000000;
+		case 0x07:
+		case 0x17:
+			return 384000000;
+		case 0x15:
+		case 0x1d:
+			return 200000000;
+		default:
+			return 320000000;
+		}
+	}
 	case BCM6368_CPU_ID:
 	{
 		unsigned int tmp, p1, p2, ndiv, m1;
@@ -205,7 +250,7 @@ static unsigned int detect_memory_size(v
 	unsigned int cols = 0, rows = 0, is_32bits = 0, banks = 0;
 	u32 val;
 
-	if (BCMCPU_IS_6328())
+	if (BCMCPU_IS_6328() || BCMCPU_IS_6362())
 		return bcm_ddr_readl(DDR_CSEND_REG) << 24;
 
 	if (BCMCPU_IS_6345()) {
@@ -280,6 +325,11 @@ void __init bcm63xx_cpu_init(void)
 				bcm63xx_regs_base = bcm6328_regs_base;
 				bcm63xx_irqs = bcm6328_irqs;
 				break;
+			case BCM6362_CPU_ID:
+				expected_cpu_id = BCM6362_CPU_ID;
+				bcm63xx_regs_base = bcm6362_regs_base;
+				bcm63xx_irqs = bcm6362_irqs;
+				break;
 			case BCM6368_CPU_ID:
 				expected_cpu_id = BCM6368_CPU_ID;
 				bcm63xx_regs_base = bcm6368_regs_base;
--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -82,6 +82,14 @@ static void __internal_irq_unmask_64(uns
 #define ext_irq_cfg_reg1	PERF_EXTIRQ_CFG_REG_6358
 #define ext_irq_cfg_reg2	0
 #endif
+#ifdef CONFIG_BCM63XX_CPU_6362
+#define irq_stat_reg		PERF_IRQSTAT_6362_REG
+#define irq_mask_reg		PERF_IRQMASK_6362_REG
+#define irq_bits		64
+#define is_ext_irq_cascaded	1
+#define ext_irq_start		(BCM_6362_EXT_IRQ0 - IRQ_INTERNAL_BASE)
+#define ext_irq_end		(BCM_6362_EXT_IRQ3 - IRQ_INTERNAL_BASE)
+#endif
 #ifdef CONFIG_BCM63XX_CPU_6368
 #define irq_stat_reg		PERF_IRQSTAT_6368_REG
 #define irq_mask_reg		PERF_IRQMASK_6368_REG
@@ -170,6 +178,16 @@ static void bcm63xx_init_irq(void)
 		ext_irq_end = BCM_6358_EXT_IRQ3 - IRQ_INTERNAL_BASE;
 		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_6358;
 		break;
+	case BCM6362_CPU_ID:
+		irq_stat_addr += PERF_IRQSTAT_6362_REG;
+		irq_mask_addr += PERF_IRQMASK_6362_REG;
+		irq_bits = 64;
+		ext_irq_count = 4;
+		is_ext_irq_cascaded = 1;
+		ext_irq_start = BCM_6362_EXT_IRQ0 - IRQ_INTERNAL_BASE;
+		ext_irq_end = BCM_6362_EXT_IRQ3 - IRQ_INTERNAL_BASE;
+		ext_irq_cfg_reg1 = PERF_EXTIRQ_CFG_REG_6362;
+		break;
 	case BCM6368_CPU_ID:
 		irq_stat_addr += PERF_IRQSTAT_6368_REG;
 		irq_mask_addr += PERF_IRQMASK_6368_REG;
@@ -457,6 +475,7 @@ static int bcm63xx_external_irq_set_type
 	case BCM6338_CPU_ID:
 	case BCM6345_CPU_ID:
 	case BCM6358_CPU_ID:
+	case BCM6362_CPU_ID:
 	case BCM6368_CPU_ID:
 		if (levelsense)
 			reg |= EXTIRQ_CFG_LEVELSENSE(irq);
--- a/arch/mips/bcm63xx/prom.c
+++ b/arch/mips/bcm63xx/prom.c
@@ -36,6 +36,8 @@ void __init prom_init(void)
 		mask = CKCTL_6348_ALL_SAFE_EN;
 	else if (BCMCPU_IS_6358())
 		mask = CKCTL_6358_ALL_SAFE_EN;
+	else if (BCMCPU_IS_6362())
+		mask = CKCTL_6362_ALL_SAFE_EN;
 	else if (BCMCPU_IS_6368())
 		mask = CKCTL_6368_ALL_SAFE_EN;
 	else
--- a/arch/mips/bcm63xx/setup.c
+++ b/arch/mips/bcm63xx/setup.c
@@ -83,6 +83,9 @@ void bcm63xx_machine_reboot(void)
 	case BCM6358_CPU_ID:
 		perf_regs[0] = PERF_EXTIRQ_CFG_REG_6358;
 		break;
+	case BCM6362_CPU_ID:
+		perf_regs[0] = PERF_EXTIRQ_CFG_REG_6362;
+		break;
 	}
 
 	for (i = 0; i < 2; i++) {
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_cpu.h
@@ -14,6 +14,7 @@
 #define BCM6345_CPU_ID		0x6345
 #define BCM6348_CPU_ID		0x6348
 #define BCM6358_CPU_ID		0x6358
+#define BCM6362_CPU_ID		0x6362
 #define BCM6368_CPU_ID		0x6368
 
 void __init bcm63xx_cpu_init(void);
@@ -86,6 +87,20 @@ unsigned int bcm63xx_get_cpu_freq(void);
 # define BCMCPU_IS_6358()	(0)
 #endif
 
+#ifdef CONFIG_BCM63XX_CPU_6362
+# ifdef bcm63xx_get_cpu_id
+#  undef bcm63xx_get_cpu_id
+#  define bcm63xx_get_cpu_id()	__bcm63xx_get_cpu_id()
+#  define BCMCPU_RUNTIME_DETECT
+# else
+#  define bcm63xx_get_cpu_id()	BCM6362_CPU_ID
+# endif
+# define BCMCPU_IS_6362()	(bcm63xx_get_cpu_id() == BCM6362_CPU_ID)
+#else
+# define BCMCPU_IS_6362()	(0)
+#endif
+
+
 #ifdef CONFIG_BCM63XX_CPU_6368
 # ifdef bcm63xx_get_cpu_id
 #  undef bcm63xx_get_cpu_id
@@ -402,6 +417,62 @@ enum bcm63xx_regs_set {
 
 
 /*
+ * 6362 register sets base address
+ */
+#define BCM_6362_DSL_LMEM_BASE		(0xdeadbeef)
+#define BCM_6362_PERF_BASE		(0xb0000000)
+#define BCM_6362_TIMER_BASE		(0xb0000040)
+#define BCM_6362_WDT_BASE		(0xb000005c)
+#define BCM_6362_UART0_BASE             (0xb0000100)
+#define BCM_6362_UART1_BASE		(0xb0000120)
+#define BCM_6362_GPIO_BASE		(0xb0000080)
+#define BCM_6362_SPI_BASE		(0xb0000800)
+#define BCM_6362_HSSPI_BASE		(0xb0001000)
+#define BCM_6362_UDC0_BASE		(0xdeadbeef)
+#define BCM_6362_USBDMA_BASE		(0xb000c000)
+#define BCM_6362_OHCI0_BASE		(0xb0002600)
+#define BCM_6362_OHCI_PRIV_BASE		(0xdeadbeef)
+#define BCM_6362_USBH_PRIV_BASE		(0xb0002700)
+#define BCM_6362_USBD_BASE		(0xb0002400)
+#define BCM_6362_MPI_BASE		(0xdeadbeef)
+#define BCM_6362_PCMCIA_BASE		(0xdeadbeef)
+#define BCM_6362_PCIE_BASE		(0xb0e40000)
+#define BCM_6362_SDRAM_REGS_BASE	(0xdeadbeef)
+#define BCM_6362_DSL_BASE		(0xdeadbeef)
+#define BCM_6362_UBUS_BASE		(0xdeadbeef)
+#define BCM_6362_ENET0_BASE		(0xdeadbeef)
+#define BCM_6362_ENET1_BASE		(0xdeadbeef)
+#define BCM_6362_ENETDMA_BASE		(0xb000d800)
+#define BCM_6362_ENETDMAC_BASE		(0xb000da00)
+#define BCM_6362_ENETDMAS_BASE		(0xb000dc00)
+#define BCM_6362_ENETSW_BASE		(0xb0e00000)
+#define BCM_6362_EHCI0_BASE		(0xb0002500)
+#define BCM_6362_SDRAM_BASE		(0xdeadbeef)
+#define BCM_6362_MEMC_BASE		(0xdeadbeef)
+#define BCM_6362_DDR_BASE		(0xb0003000)
+#define BCM_6362_M2M_BASE		(0xdeadbeef)
+#define BCM_6362_ATM_BASE		(0xdeadbeef)
+#define BCM_6362_XTM_BASE		(0xb0007800)
+#define BCM_6362_XTMDMA_BASE		(0xb000b800)
+#define BCM_6362_XTMDMAC_BASE		(0xdeadbeef)
+#define BCM_6362_XTMDMAS_BASE		(0xdeadbeef)
+#define BCM_6362_PCM_BASE		(0xb000a800)
+#define BCM_6362_PCMDMA_BASE		(0xdeadbeef)
+#define BCM_6362_PCMDMAC_BASE		(0xdeadbeef)
+#define BCM_6362_PCMDMAS_BASE		(0xdeadbeef)
+#define BCM_6362_RNG_BASE		(0xdeadbeef)
+#define BCM_6362_MISC_BASE		(0xb0001800)
+
+#define BCM_6362_NAND_REG_BASE		(0xb0000200)
+#define BCM_6362_NAND_CACHE_BASE	(0xb0000600)
+#define BCM_6362_LED_BASE		(0xb0001900)
+#define BCM_6362_IPSEC_BASE		(0xb0002800)
+#define BCM_6362_IPSEC_DMA_BASE		(0xb000d000)
+#define BCM_6362_WLAN_CHIPCOMMON_BASE	(0xb0004000)
+#define BCM_6362_WLAN_D11_BASE		(0xb0005000)
+#define BCM_6362_WLAN_SHIM_BASE		(0xb0007000)
+
+/*
  * 6368 register sets base address
  */
 #define BCM_6368_DSL_LMEM_BASE		(0xdeadbeef)
@@ -557,6 +628,9 @@ static inline unsigned long bcm63xx_regs
 #ifdef CONFIG_BCM63XX_CPU_6358
 	__GEN_RSET(6358)
 #endif
+#ifdef CONFIG_BCM63XX_CPU_6362
+	__GEN_RSET(6362)
+#endif
 #ifdef CONFIG_BCM63XX_CPU_6368
 	__GEN_RSET(6368)
 #endif
@@ -777,6 +851,71 @@ enum bcm63xx_irq {
 #define BCM_6358_EXT_IRQ3		(IRQ_INTERNAL_BASE + 28)
 
 /*
+ * 6362 irqs
+ */
+#define BCM_6362_HIGH_IRQ_BASE		(IRQ_INTERNAL_BASE + 32)
+
+#define BCM_6362_TIMER_IRQ		(IRQ_INTERNAL_BASE + 0)
+#define BCM_6362_SPI_IRQ		(IRQ_INTERNAL_BASE + 2)
+#define BCM_6362_UART0_IRQ		(IRQ_INTERNAL_BASE + 3)
+#define BCM_6362_UART1_IRQ		(IRQ_INTERNAL_BASE + 4)
+#define BCM_6362_DSL_IRQ		(IRQ_INTERNAL_BASE + 28)
+#define BCM_6362_UDC0_IRQ		0
+#define BCM_6362_ENET0_IRQ		0
+#define BCM_6362_ENET1_IRQ		0
+#define BCM_6362_ENET_PHY_IRQ		(IRQ_INTERNAL_BASE + 14)
+#define BCM_6362_HSSPI_IRQ		(IRQ_INTERNAL_BASE + 5)
+#define BCM_6362_OHCI0_IRQ		(IRQ_INTERNAL_BASE + 9)
+#define BCM_6362_EHCI0_IRQ		(IRQ_INTERNAL_BASE + 10)
+#define BCM_6362_USBD_IRQ		(IRQ_INTERNAL_BASE + 11)
+#define BCM_6362_USBD_RXDMA0_IRQ	(IRQ_INTERNAL_BASE + 20)
+#define BCM_6362_USBD_TXDMA0_IRQ	(IRQ_INTERNAL_BASE + 21)
+#define BCM_6362_USBD_RXDMA1_IRQ	(IRQ_INTERNAL_BASE + 22)
+#define BCM_6362_USBD_TXDMA1_IRQ	(IRQ_INTERNAL_BASE + 23)
+#define BCM_6362_USBD_RXDMA2_IRQ	(IRQ_INTERNAL_BASE + 24)
+#define BCM_6362_USBD_TXDMA2_IRQ	(IRQ_INTERNAL_BASE + 25)
+#define BCM_6362_PCMCIA_IRQ		0
+#define BCM_6362_ENET0_RXDMA_IRQ	0
+#define BCM_6362_ENET0_TXDMA_IRQ	0
+#define BCM_6362_ENET1_RXDMA_IRQ	0
+#define BCM_6362_ENET1_TXDMA_IRQ	0
+#define BCM_6362_PCI_IRQ		(IRQ_INTERNAL_BASE + 30)
+#define BCM_6362_ATM_IRQ		0
+#define BCM_6362_ENETSW_RXDMA0_IRQ	(BCM_6362_HIGH_IRQ_BASE + 0)
+#define BCM_6362_ENETSW_RXDMA1_IRQ	(BCM_6362_HIGH_IRQ_BASE + 1)
+#define BCM_6362_ENETSW_RXDMA2_IRQ	(BCM_6362_HIGH_IRQ_BASE + 2)
+#define BCM_6362_ENETSW_RXDMA3_IRQ	(BCM_6362_HIGH_IRQ_BASE + 3)
+#define BCM_6362_ENETSW_TXDMA0_IRQ	0
+#define BCM_6362_ENETSW_TXDMA1_IRQ	0
+#define BCM_6362_ENETSW_TXDMA2_IRQ	0
+#define BCM_6362_ENETSW_TXDMA3_IRQ	0
+#define BCM_6362_XTM_IRQ		0
+#define BCM_6362_XTM_DMA0_IRQ		(BCM_6362_HIGH_IRQ_BASE + 12)
+
+#define BCM_6362_RING_OSC_IRQ		(IRQ_INTERNAL_BASE + 1)
+#define BCM_6362_WLAN_GPIO_IRQ		(IRQ_INTERNAL_BASE + 6)
+#define BCM_6362_WLAN_IRQ		(IRQ_INTERNAL_BASE + 7)
+#define BCM_6362_IPSEC_IRQ		(IRQ_INTERNAL_BASE + 8)
+#define BCM_6362_NAND_IRQ		(IRQ_INTERNAL_BASE + 12)
+#define BCM_6362_PCM_IRQ		(IRQ_INTERNAL_BASE + 13)
+#define BCM_6362_DG_IRQ			(IRQ_INTERNAL_BASE + 15)
+#define BCM_6362_EPHY_ENERGY0_IRQ	(IRQ_INTERNAL_BASE + 16)
+#define BCM_6362_EPHY_ENERGY1_IRQ	(IRQ_INTERNAL_BASE + 17)
+#define BCM_6362_EPHY_ENERGY2_IRQ	(IRQ_INTERNAL_BASE + 18)
+#define BCM_6362_EPHY_ENERGY3_IRQ	(IRQ_INTERNAL_BASE + 19)
+#define BCM_6362_IPSEC_DMA0_IRQ		(IRQ_INTERNAL_BASE + 26)
+#define BCM_6362_IPSEC_DMA1_IRQ		(IRQ_INTERNAL_BASE + 27)
+#define BCM_6362_FAP0_IRQ		(IRQ_INTERNAL_BASE + 29)
+#define BCM_6362_PCM_DMA0_IRQ		(BCM_6362_HIGH_IRQ_BASE + 4)
+#define BCM_6362_PCM_DMA1_IRQ		(BCM_6362_HIGH_IRQ_BASE + 5)
+#define BCM_6362_DECT0_IRQ		(BCM_6362_HIGH_IRQ_BASE + 6)
+#define BCM_6362_DECT1_IRQ		(BCM_6362_HIGH_IRQ_BASE + 7)
+#define BCM_6362_EXT_IRQ0		(BCM_6362_HIGH_IRQ_BASE + 8)
+#define BCM_6362_EXT_IRQ1		(BCM_6362_HIGH_IRQ_BASE + 9)
+#define BCM_6362_EXT_IRQ2		(BCM_6362_HIGH_IRQ_BASE + 10)
+#define BCM_6362_EXT_IRQ3		(BCM_6362_HIGH_IRQ_BASE + 11)
+
+/*
  * 6368 irqs
  */
 #define BCM_6368_HIGH_IRQ_BASE		(IRQ_INTERNAL_BASE + 32)
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_gpio.h
@@ -17,6 +17,8 @@ static inline unsigned long bcm63xx_gpio
 		return 8;
 	case BCM6345_CPU_ID:
 		return 16;
+	case BCM6362_CPU_ID:
+		return 48;
 	case BCM6368_CPU_ID:
 		return 38;
 	case BCM6348_CPU_ID:
--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
@@ -107,6 +107,39 @@
 					CKCTL_6358_USBSU_EN |		\
 					CKCTL_6358_EPHY_EN)
 
+#define CKCTL_6362_ADSL_QPROC_EN	(1 << 1)
+#define CKCTL_6362_ADSL_AFE_EN		(1 << 2)
+#define CKCTL_6362_ADSL_EN		(1 << 3)
+#define CKCTL_6362_MIPS_EN		(1 << 4)
+#define CKCTL_6362_WLAN_OCP_EN		(1 << 5)
+#define CKCTL_6362_SWPKT_USB_EN		(1 << 7)
+#define CKCTL_6362_SWPKT_SAR_EN		(1 << 8)
+#define CKCTL_6362_SAR_EN		(1 << 9)
+#define CKCTL_6362_ROBOSW_EN		(1 << 10)
+#define CKCTL_6362_PCM_EN		(1 << 11)
+#define CKCTL_6362_USBD_EN		(1 << 12)
+#define CKCTL_6362_USBH_EN		(1 << 13)
+#define CKCTL_6362_IPSEC_EN		(1 << 14)
+#define CKCTL_6362_SPI_EN		(1 << 15)
+#define CKCTL_6362_HSSPI_EN		(1 << 16)
+#define CKCTL_6362_PCIE_EN		(1 << 17)
+#define CKCTL_6362_FAP_EN		(1 << 18)
+#define CKCTL_6362_PHYMIPS_EN		(1 << 19)
+#define CKCTL_6362_NAND_EN		(1 << 20)
+
+#define CKCTL_6362_ALL_SAFE_EN		(CKCTL_6362_PHYMIPS_EN |	\
+					CKCTL_6362_ADSL_QPROC_EN |	\
+					CKCTL_6362_ADSL_AFE_EN |	\
+					CKCTL_6362_ADSL_EN |		\
+					CKCTL_6362_SAR_EN  |		\
+					CKCTL_6362_PCM_EN  |		\
+					CKCTL_6362_IPSEC_EN |		\
+					CKCTL_6362_USBD_EN |		\
+					CKCTL_6362_USBH_EN |		\
+					CKCTL_6362_ROBOSW_EN |		\
+					CKCTL_6362_PCIE_EN)
+
+
 #define CKCTL_6368_VDSL_QPROC_EN	(1 << 2)
 #define CKCTL_6368_VDSL_AFE_EN		(1 << 3)
 #define CKCTL_6368_VDSL_BONDING_EN	(1 << 4)
@@ -148,6 +181,7 @@
 #define PERF_IRQMASK_6345_REG		0xc
 #define PERF_IRQMASK_6348_REG		0xc
 #define PERF_IRQMASK_6358_REG		0xc
+#define PERF_IRQMASK_6362_REG		0x20
 #define PERF_IRQMASK_6368_REG		0x20
 
 /* Interrupt Status register */
@@ -156,6 +190,7 @@
 #define PERF_IRQSTAT_6345_REG		0x10
 #define PERF_IRQSTAT_6348_REG		0x10
 #define PERF_IRQSTAT_6358_REG		0x10
+#define PERF_IRQSTAT_6362_REG		0x28
 #define PERF_IRQSTAT_6368_REG		0x28
 
 /* External Interrupt Configuration register */
@@ -164,6 +199,7 @@
 #define PERF_EXTIRQ_CFG_REG_6345	0x14
 #define PERF_EXTIRQ_CFG_REG_6348	0x14
 #define PERF_EXTIRQ_CFG_REG_6358	0x14
+#define PERF_EXTIRQ_CFG_REG_6362	0x18
 #define PERF_EXTIRQ_CFG_REG_6368	0x18
 
 #define PERF_EXTIRQ_CFG_REG2_6368	0x1c
@@ -191,6 +227,7 @@
 /* Soft Reset register */
 #define PERF_SOFTRESET_REG		0x28
 #define PERF_SOFTRESET_6328_REG		0x10
+#define PERF_SOFTRESET_6362_REG		0x10
 #define PERF_SOFTRESET_6368_REG		0x10
 
 #define SOFTRESET_6328_SPI_MASK		(1 << 0)
@@ -244,6 +281,22 @@
 				  SOFTRESET_6348_ACLC_MASK |		\
 				  SOFTRESET_6348_ADSLMIPSPLL_MASK)
 
+#define SOFTRESET_6362_SPI_MASK		(1 << 0)
+#define SOFTRESET_6362_IPSEC_MASK	(1 << 1)
+#define SOFTRESET_6362_EPHY_MASK	(1 << 2)
+#define SOFTRESET_6362_SAR_MASK		(1 << 3)
+#define SOFTRESET_6362_ENETSW_MASK	(1 << 4)
+#define SOFTRESET_6362_USBS_MASK	(1 << 5)
+#define SOFTRESET_6362_USBH_MASK	(1 << 6)
+#define SOFTRESET_6362_PCM_MASK		(1 << 7)
+#define SOFTRESET_6362_PCIE_CORE_MASK	(1 << 8)
+#define SOFTRESET_6362_PCIE_MASK	(1 << 9)
+#define SOFTRESET_6362_PCIE_EXT_MASK	(1 << 10)
+#define SOFTRESET_6362_WLAN_SHIM_MASK	(1 << 11)
+#define SOFTRESET_6362_DDR_PHY_MASK	(1 << 12)
+#define SOFTRESET_6362_FAP_MASK		(1 << 13)
+#define SOFTRESET_6362_WLAN_UBUS_MASK	(1 << 14)
+
 #define SOFTRESET_6368_SPI_MASK		(1 << 0)
 #define SOFTRESET_6368_MPI_MASK		(1 << 3)
 #define SOFTRESET_6368_EPHY_MASK	(1 << 6)
@@ -1182,6 +1235,12 @@
 #define SERDES_PCIE_EN			(1 << 0)
 #define SERDES_PCIE_EXD_EN		(1 << 15)
 
+#define MISC_STRAPBUS_6362_REG		0x14
+#define STRAPBUS_6362_FCVO_SHIFT	1
+#define STRAPBUS_6362_FCVO_MASK		(0x1f << STRAPBUS_6362_FCVO_SHIFT)
+#define STRAPBUS_6362_BOOT_SEL_SERIAL	(1 << 15)
+#define STRAPBUS_6362_BOOT_SEL_NAND	(0 << 15)
+
 #define MISC_STRAPBUS_6328_REG		0x240
 #define STRAPBUS_6328_FCVO_SHIFT	7
 #define STRAPBUS_6328_FCVO_MASK		(0x1f << STRAPBUS_6328_FCVO_SHIFT)
--- a/arch/mips/include/asm/mach-bcm63xx/ioremap.h
+++ b/arch/mips/include/asm/mach-bcm63xx/ioremap.h
@@ -19,6 +19,7 @@ static inline int is_bcm63xx_internal_re
 			return 1;
 		break;
 	case BCM6328_CPU_ID:
+	case BCM6362_CPU_ID:
 	case BCM6368_CPU_ID:
 		if (offset >= 0xb0000000 && offset < 0xb1000000)
 			return 1;
