--- a/drivers/net/wireless/brcm80211/brcmsmac/mac80211_if.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/mac80211_if.c
@@ -94,6 +94,7 @@ MODULE_FIRMWARE("brcm/bcm43xx_hdr-0.fw")
 
 /* recognized BCMA Core IDs */
 static struct bcma_device_id brcms_coreid_table[] = {
+//	BCMA_CORE(BCMA_MANUF_BCM, BCMA_CORE_80211, 17, BCMA_ANY_CLASS),
 	BCMA_CORE(BCMA_MANUF_BCM, BCMA_CORE_80211, 23, BCMA_ANY_CLASS),
 	BCMA_CORE(BCMA_MANUF_BCM, BCMA_CORE_80211, 24, BCMA_ANY_CLASS),
 	BCMA_CORETABLE_END
--- a/drivers/net/wireless/brcm80211/brcmsmac/main.c
+++ b/drivers/net/wireless/brcm80211/brcmsmac/main.c
@@ -734,7 +734,7 @@ static void brcms_c_ucode_bsinit(struct 
 	brcms_c_write_mhf(wlc_hw, wlc_hw->band->mhfs);
 
 	/* do band-specific ucode IHR, SHM, and SCR inits */
-	if (D11REV_IS(wlc_hw->corerev, 23)) {
+	if (D11REV_IS(wlc_hw->corerev, 17) || D11REV_IS(wlc_hw->corerev, 23)) {
 		if (BRCMS_ISNPHY(wlc_hw->band))
 			brcms_c_write_inits(wlc_hw, ucode->d11n0bsinitvals16);
 		else
@@ -2259,7 +2259,7 @@ static void brcms_ucode_download(struct 
 	if (wlc_hw->ucode_loaded)
 		return;
 
-	if (D11REV_IS(wlc_hw->corerev, 23)) {
+	if (D11REV_IS(wlc_hw->corerev, 17) || D11REV_IS(wlc_hw->corerev, 23)) {
 		if (BRCMS_ISNPHY(wlc_hw->band)) {
 			brcms_ucode_write(wlc_hw, ucode->bcm43xx_16_mimo,
 					  ucode->bcm43xx_16_mimosz);
@@ -3221,7 +3221,7 @@ static void brcms_b_coreinit(struct brcm
 
 	sflags = bcma_aread32(core, BCMA_IOST);
 
-	if (D11REV_IS(wlc_hw->corerev, 23)) {
+	if (D11REV_IS(wlc_hw->corerev, 17) || D11REV_IS(wlc_hw->corerev, 23)) {
 		if (BRCMS_ISNPHY(wlc_hw->band))
 			brcms_c_write_inits(wlc_hw, ucode->d11n0initvals16);
 		else
