--- a/include/linux/spi/spi.h
+++ b/include/linux/spi/spi.h
@@ -503,6 +503,8 @@ struct spi_transfer {
 	dma_addr_t	rx_dma;
 
 	unsigned	cs_change:1;
+	unsigned	verify:1;
+	unsigned	fast_write:1;
 	u8		bits_per_word;
 	u16		delay_usecs;
 	u32		speed_hz;
@@ -544,6 +546,7 @@ struct spi_message {
 	struct spi_device	*spi;
 
 	unsigned		is_dma_mapped:1;
+	unsigned		fast_read:1;
 
 	/* REVISIT:  we might want a flag affecting the behavior of the
 	 * last transfer ... allowing things like "read 16 bit length L"
