From 0f5728e7e6fa7f0969ec79bd623261d3d830e5e7 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 14 Mar 2012 10:29:27 +0100
Subject: [PATCH 11/47] MIPS: ath79: use io-accessor macros in pci-ar724x.c
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Acked-by: René Bolldorf <xsecute@googlemail.com>
Cc: linux-mips@linux-mips.org
Patchwork: https://patchwork.linux-mips.org/patch/3491/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/pci/pci-ar724x.c |   38 ++++++++++++++++++++++++--------------
 1 files changed, 24 insertions(+), 14 deletions(-)

--- a/arch/mips/pci/pci-ar724x.c
+++ b/arch/mips/pci/pci-ar724x.c
@@ -11,19 +11,19 @@
 #include <linux/pci.h>
 #include <asm/mach-ath79/pci.h>
 
-#define reg_read(_phys)		(*(unsigned int *) KSEG1ADDR(_phys))
-#define reg_write(_phys, _val)	((*(unsigned int *) KSEG1ADDR(_phys)) = (_val))
-
-#define AR724X_PCI_DEV_BASE	0x14000000
+#define AR724X_PCI_CFG_BASE	0x14000000
+#define AR724X_PCI_CFG_SIZE	0x1000
 #define AR724X_PCI_MEM_BASE	0x10000000
 #define AR724X_PCI_MEM_SIZE	0x08000000
 
 static DEFINE_SPINLOCK(ar724x_pci_lock);
+static void __iomem *ar724x_pci_devcfg_base;
 
 static int ar724x_pci_read(struct pci_bus *bus, unsigned int devfn, int where,
 			    int size, uint32_t *value)
 {
 	unsigned long flags, addr, tval, mask;
+	void __iomem *base;
 
 	if (devfn)
 		return PCIBIOS_DEVICE_NOT_FOUND;
@@ -31,25 +31,27 @@ static int ar724x_pci_read(struct pci_bu
 	if (where & (size - 1))
 		return PCIBIOS_BAD_REGISTER_NUMBER;
 
+	base = ar724x_pci_devcfg_base;
+
 	spin_lock_irqsave(&ar724x_pci_lock, flags);
 
 	switch (size) {
 	case 1:
 		addr = where & ~3;
 		mask = 0xff000000 >> ((where % 4) * 8);
-		tval = reg_read(AR724X_PCI_DEV_BASE + addr);
+		tval = __raw_readl(base + addr);
 		tval = tval & ~mask;
 		*value = (tval >> ((4 - (where % 4))*8));
 		break;
 	case 2:
 		addr = where & ~3;
 		mask = 0xffff0000 >> ((where % 4)*8);
-		tval = reg_read(AR724X_PCI_DEV_BASE + addr);
+		tval = __raw_readl(base + addr);
 		tval = tval & ~mask;
 		*value = (tval >> ((4 - (where % 4))*8));
 		break;
 	case 4:
-		*value = reg_read(AR724X_PCI_DEV_BASE + where);
+		*value = __raw_readl(base + where);
 		break;
 	default:
 		spin_unlock_irqrestore(&ar724x_pci_lock, flags);
@@ -66,6 +68,7 @@ static int ar724x_pci_write(struct pci_b
 			     int size, uint32_t value)
 {
 	unsigned long flags, tval, addr, mask;
+	void __iomem *base;
 
 	if (devfn)
 		return PCIBIOS_DEVICE_NOT_FOUND;
@@ -73,27 +76,29 @@ static int ar724x_pci_write(struct pci_b
 	if (where & (size - 1))
 		return PCIBIOS_BAD_REGISTER_NUMBER;
 
+	base = ar724x_pci_devcfg_base;
+
 	spin_lock_irqsave(&ar724x_pci_lock, flags);
 
 	switch (size) {
 	case 1:
-		addr = (AR724X_PCI_DEV_BASE + where) & ~3;
+		addr = where & ~3;
 		mask = 0xff000000 >> ((where % 4)*8);
-		tval = reg_read(addr);
+		tval = __raw_readl(base + addr);
 		tval = tval & ~mask;
 		tval |= (value << ((4 - (where % 4))*8)) & mask;
-		reg_write(addr, tval);
+		__raw_writel(tval, base + addr);
 		break;
 	case 2:
-		addr = (AR724X_PCI_DEV_BASE + where) & ~3;
+		addr = where & ~3;
 		mask = 0xffff0000 >> ((where % 4)*8);
-		tval = reg_read(addr);
+		tval = __raw_readl(base + addr);
 		tval = tval & ~mask;
 		tval |= (value << ((4 - (where % 4))*8)) & mask;
-		reg_write(addr, tval);
+		__raw_writel(tval, base + addr);
 		break;
 	case 4:
-		reg_write((AR724X_PCI_DEV_BASE + where), value);
+		__raw_writel(value, (base + where));
 		break;
 	default:
 		spin_unlock_irqrestore(&ar724x_pci_lock, flags);
@@ -133,6 +138,11 @@ static struct pci_controller ar724x_pci_
 
 int __init ar724x_pcibios_init(void)
 {
+	ar724x_pci_devcfg_base = ioremap(AR724X_PCI_CFG_BASE,
+					 AR724X_PCI_CFG_SIZE);
+	if (ar724x_pci_devcfg_base == NULL)
+		return -ENOMEM;
+
 	register_pci_controller(&ar724x_pci_controller);
 
 	return PCIBIOS_SUCCESSFUL;
