--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -328,6 +328,14 @@ config USB_OHCI_ATH79
 	  Enables support for the built-in OHCI controller present on the
 	  Atheros AR71XX/AR7240 SoCs.
 
+config USB_OHCI_RT3883
+	bool "USB OHCI support for the Ralink RT3883 SoCs"
+	depends on USB_OHCI_HCD && ( SOC_RT3883 || SOC_RT305X )
+	default y
+	help
+	  Enables support for the built-in OHCI controller present on the
+	  Ralink RT3883 SoC.
+
 config USB_OHCI_HCD_PPC_SOC
 	bool "OHCI support for on-chip PPC USB controller"
 	depends on USB_OHCI_HCD && (STB03xxx || PPC_MPC52xx)
--- a/drivers/usb/host/ohci-hcd.c
+++ b/drivers/usb/host/ohci-hcd.c
@@ -1121,6 +1121,11 @@ MODULE_LICENSE ("GPL");
 #define PLATFORM_DRIVER		ohci_xls_driver
 #endif
 
+#ifdef CONFIG_USB_OHCI_RT3883
+#include "ohci-rt3883.c"
+#define PLATFORM_DRIVER		ohci_rt3883_driver
+#endif
+
 #if	!defined(PCI_DRIVER) &&		\
 	!defined(PLATFORM_DRIVER) &&	\
 	!defined(OMAP1_PLATFORM_DRIVER) &&	\
