From adb6abbe4e3bc17c20cdc70e4a4357f1633d4970 Mon Sep 17 00:00:00 2001
From: Joseph Kortje <jpktech@rogers.com>
Date: Wed, 28 Oct 2009 21:49:11 -0400
Subject: [PATCH] [ARM] gumstix.h: Verdex Pro support

Added a bunch of ifdefs to support both original gumstix boards
as well as the Verdex Pro in gumstix.h

Signed-off-by: Bobby Powers <bobbypowers@gmail.com>
---
 arch/arm/mach-pxa/include/mach/gumstix.h |  160 ++++++++++++++++++++++++------
 1 files changed, 130 insertions(+), 30 deletions(-)

--- a/arch/arm/mach-pxa/include/mach/gumstix.h
+++ b/arch/arm/mach-pxa/include/mach/gumstix.h
@@ -6,6 +6,9 @@
  * published by the Free Software Foundation.
  */
 
+#if !defined(__ASM_ARCH_MFP_PXA27X_H) && !defined(__ASM_ARCH_MFP_PXA25X_H)
+	#error You need to include either mfp-pxa27x.h or mfp-pxa25x.h
+#endif
 
 /* BTRESET - Reset line to Bluetooth module, active low signal. */
 #define GPIO_GUMSTIX_BTRESET          7
@@ -20,9 +23,18 @@ this moves to GPIO17 and GPIO37. */
 /* GPIOx - Connects to USB D+ and used as a pull-up after GPIOn
 has detected a cable insertion; driven low otherwise. */
 
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
+
 #define GPIO_GUMSTIX_USB_GPIOn		35
 #define GPIO_GUMSTIX_USB_GPIOx		41
 
+#else
+
+#define GPIO_GUMSTIX_USB_GPIOn         100
+#define GPIO_GUMSTIX_USB_GPIOx         27
+
+#endif
+
 /* usb state change */
 #define GUMSTIX_USB_INTR_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_USB_GPIOn)
 
@@ -42,48 +54,136 @@ has detected a cable insertion; driven l
  * ETH_RST provides a hardware reset line to the ethernet chip
  * ETH is the IRQ line in from the ethernet chip to the PXA
  */
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
 #define GPIO_GUMSTIX_ETH0_RST		80
-#define GPIO_GUMSTIX_ETH0_RST_MD	(GPIO_GUMSTIX_ETH0_RST | GPIO_OUT)
+#define GPIO_GUMSTIX_ETH0		36
+#else
+#define GPIO_GUMSTIX_ETH0_RST		107
+#define GPIO_GUMSTIX_ETH0		99
+#endif
 #define GPIO_GUMSTIX_ETH1_RST		52
-#define GPIO_GUMSTIX_ETH1_RST_MD	(GPIO_GUMSTIX_ETH1_RST | GPIO_OUT)
+#define GPIO_GUMSTIX_ETH1		27
 
-#define GPIO_GUMSTIX_ETH0		36
+#define GPIO_GUMSTIX_ETH0_RST_MD	(GPIO_GUMSTIX_ETH0_RST | GPIO_OUT)
+#define GPIO_GUMSTIX_ETH1_RST_MD	(GPIO_GUMSTIX_ETH1_RST | GPIO_OUT)
 #define GPIO_GUMSTIX_ETH0_MD		(GPIO_GUMSTIX_ETH0 | GPIO_IN)
-#define GUMSTIX_ETH0_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_ETH0)
-#define GPIO_GUMSTIX_ETH1		27
 #define GPIO_GUMSTIX_ETH1_MD		(GPIO_GUMSTIX_ETH1 | GPIO_IN)
-#define GUMSTIX_ETH1_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_ETH1)
-
 
-/* CF reset line */
-#define GPIO8_RESET			8
+#define GUMSTIX_ETH0_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_ETH0)
+#define GUMSTIX_ETH1_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_ETH1)
 
-/* CF slot 0 */
-#define GPIO4_nBVD1			4
-#define GPIO4_nSTSCHG			GPIO4_nBVD1
-#define GPIO11_nCD			11
-#define GPIO26_PRDY_nBSY		26
-#define GUMSTIX_S0_nSTSCHG_IRQ		PXA_GPIO_TO_IRQ(GPIO4_nSTSCHG)
-#define GUMSTIX_S0_nCD_IRQ		PXA_GPIO_TO_IRQ(GPIO11_nCD)
-#define GUMSTIX_S0_PRDY_nBSY_IRQ	PXA_GPIO_TO_IRQ(GPIO26_PRDY_nBSY)
+ /* CF reset line */
+#define GPIO8_CF_RESET			8
+#define GPIO97_CF_RESET			97
+#define GPIO110_CF_RESET		110
+
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
+#define GPIO_GUMSTIX_CF_RESET		GPIO8_CF_RESET
+#else
+#define GPIO_GUMSTIX_CF_RESET		GPIO97_CF_RESET
+#endif
+
+#define GPIO_GUMSTIX_CF_OLD_RESET	GPIO110_CF_RESET
+
+/* CF signals shared by both sockets */
+#define GPIO_GUMSTIX_nPOE	48
+#define GPIO_GUMSTIX_nPWE	49
+#define GPIO_GUMSTIX_nPIOR	50
+#define GPIO_GUMSTIX_nPIOW	51
+
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
+#define GPIO_GUMSTIX_nPCE_1	52
+#define GPIO_GUMSTIX_nPCE_2	53
+#define GPIO_GUMSTIX_pSKTSEL	54
+#else
+#define GPIO_GUMSTIX_nPCE_1	102
+#define GPIO_GUMSTIX_nPCE_2	105
+#define GPIO_GUMSTIX_pSKTSEL	79
+#endif
+
+#define GPIO_GUMSTIX_nPREG	55
+#define GPIO_GUMSTIX_nPWAIT	56
+#define GPIO_GUMSTIX_nIOIS16	57
+
+/* Pin mode definitions correspond to mfp-pxa2[57]x.h */
+#define GPIO_GUMSTIX_nPOE_MD	GPIO48_nPOE
+#define GPIO_GUMSTIX_nPWE_MD	GPIO49_nPWE
+#define GPIO_GUMSTIX_nPIOR_MD	GPIO50_nPIOR
+#define GPIO_GUMSTIX_nPIOW_MD	GPIO51_nPIOW
+
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
+#define GPIO_GUMSTIX_nPCE_1_MD	GPIO52_nPCE_1
+#define GPIO_GUMSTIX_nPCE_2_MD	GPIO53_nPCE_2
+#define GPIO_GUMSTIX_pSKTSEL_MD	GPIO54_pSKTSEL
+#else
+#define GPIO_GUMSTIX_nPCE_1_MD	GPIO102_nPCE_1
+#define GPIO_GUMSTIX_nPCE_2_MD	GPIO105_nPCE_2
+#define GPIO_GUMSTIX_pSKTSEL_MD	GPIO79_pSKTSEL
+#endif
+
+#define GPIO_GUMSTIX_nPREG_MD	GPIO55_nPREG
+#define GPIO_GUMSTIX_nPWAIT_MD	GPIO56_nPWAIT
+#define GPIO_GUMSTIX_nIOIS16_MD	GPIO57_nIOIS16
+
+ /* CF slot 0 */
+#define GPIO4_nBVD1_0			4
+#define GPIO4_nSTSCHG_0			GPIO4_nBVD1_0
+#define GPIO11_nCD_0			11
+#define GPIO26_PRDY_nBSY_0		26
+
+#define GPIO111_nBVD1_0			111
+#define GPIO111_nSTSCHG_0		GPIO111_nBVD1_0
+#define GPIO104_nCD_0			104
+#define GPIO96_PRDY_nBSY_0		96
+#define GPIO109_PRDY_nBSY_0		109
+
+#ifndef CONFIG_MACH_GUMSTIX_VERDEX
+#define GPIO_GUMSTIX_nBVD1_0		GPIO4_nBVD1_0
+#define GPIO_GUMSTIX_nSTSCHG_0		GPIO4_nSTSCHG_0
+#define GPIO_GUMSTIX_nCD_0		GPIO11_nCD_0
+#define GPIO_GUMSTIX_PRDY_nBSY_0	GPIO26_PRDY_nBSY_0
+#else
+#define GPIO_GUMSTIX_nBVD1_0		GPIO111_nBVD1_0
+#define GPIO_GUMSTIX_nSTSCHG_0		GPIO111_nSTSCHG_0
+#define GPIO_GUMSTIX_nCD_0		GPIO104_nCD_0
+#define GPIO_GUMSTIX_PRDY_nBSY_0	GPIO96_PRDY_nBSY_0
+#endif
+
+#define GPIO_GUMSTIX_PRDY_nBSY_0_OLD	GPIO109_PRDY_nBSY_0
+#define GUMSTIX_S0_PRDY_nBSY_OLD_IRQ	PXA_GPIO_TO_IRQ(GPIO109_PRDY_nBSY_0)
+
+#define GUMSTIX_S0_nSTSCHG_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_nSTSCHG_0)
+#define GUMSTIX_S0_nCD_IRQ		PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_nCD_0)
+#define GUMSTIX_S0_PRDY_nBSY_IRQ	PXA_GPIO_TO_IRQ(GPIO_GUMSTIX_PRDY_nBSY_0)
 
 /* CF slot 1 */
-#define GPIO18_nBVD1			18
-#define GPIO18_nSTSCHG			GPIO18_nBVD1
-#define GPIO36_nCD			36
-#define GPIO27_PRDY_nBSY		27
-#define GUMSTIX_S1_nSTSCHG_IRQ		PXA_GPIO_TO_IRQ(GPIO18_nSTSCHG)
-#define GUMSTIX_S1_nCD_IRQ		PXA_GPIO_TO_IRQ(GPIO36_nCD)
-#define GUMSTIX_S1_PRDY_nBSY_IRQ	PXA_GPIO_TO_IRQ(GPIO27_PRDY_nBSY)
-
-/* CF GPIO line modes */
-#define GPIO4_nSTSCHG_MD		(GPIO4_nSTSCHG | GPIO_IN)
-#define GPIO8_RESET_MD			(GPIO8_RESET | GPIO_OUT)
-#define GPIO11_nCD_MD			(GPIO11_nCD | GPIO_IN)
-#define GPIO18_nSTSCHG_MD		(GPIO18_nSTSCHG | GPIO_IN)
-#define GPIO26_PRDY_nBSY_MD		(GPIO26_PRDY_nBSY | GPIO_IN)
-#define GPIO27_PRDY_nBSY_MD		(GPIO27_PRDY_nBSY | GPIO_IN)
-#define GPIO36_nCD_MD			(GPIO36_nCD | GPIO_IN)
+#define GPIO18_nBVD1_1			18
+#define GPIO18_nSTSCHG_1		GPIO18_nBVD1_1
+#define GPIO36_nCD_1			36
+#define GPIO27_PRDY_nBSY_1		27
+
+#define GPIO_GUMSTIX_nBVD1_1		GPIO18_nBVD1_1
+#define GPIO_GUMSTIX_nSTSCHG_1		GPIO18_nSTSCHG_1
+#define GPIO_GUMSTIX_nCD_1		GPIO36_nCD_1
+#define GPIO_GUMSTIX_PRDY_nBSY_1	GPIO27_PRDY_nBSY_1
+
+#define GUMSTIX_S1_nSTSCHG_IRQ		PXA_GPIO_TO_IRQ(GPIO18_nSTSCHG_1)
+#define GUMSTIX_S1_nCD_IRQ		PXA_GPIO_TO_IRQ(GPIO36_nCD_1)
+#define GUMSTIX_S1_PRDY_nBSY_IRQ	PXA_GPIO_TO_IRQ(GPIO27_PRDY_nBSY_1)
+
+/* CF GPIO line modes - correspond to mfp-pxa2[57]x.h */
+#define GPIO_GUMSTIX_CF_RESET_MD	(GPIO_GUMSTIX_CF_RESET | GPIO_OUT)
+#define GPIO_GUMSTIX_CF_OLD_RESET_MD	(GPIO_GUMSTIX_CF_OLD_RESET | GPIO_OUT)
+
+#define GPIO_GUMSTIX_nSTSCHG_0_MD	GPIO111_GPIO
+#define GPIO_GUMSTIX_nCD_0_MD		GPIO104_GPIO
+
+#define GPIO_GUMSTIX_PRDY_nBSY_0_MD	GPIO96_GPIO
+#define GPIO_GUMSTIX_PRDY_nBSY_0_OLD_MD	GPIO109_GPIO
+
+#define GPIO_GUMSTIX_nSTSCHG_1_MD	GPIO18_GPIO
+#define GPIO_GUMSTIX_nCD_1_MD		GPIO36_GPIO
+#define GPIO_GUMSTIX_PRDY_nBSY_1_MD	GPIO27_GPIO
 
 /* for expansion boards that can't be programatically detected */
 extern int am200_init(void);
