--- a/drivers/net/phy/Kconfig
+++ b/drivers/net/phy/Kconfig
@@ -121,6 +121,11 @@ config IP17XX_PHY
 	tristate "Driver for IC+ IP17xx switches"
 	select SWCONFIG
 
+config AR8216_PHY
+	tristate "Driver for Atheros AR8216 switches"
+	select ETHERNET_PACKET_MANGLE
+	select SWCONFIG
+
 config FIXED_PHY
 	bool "Driver for MDIO Bus/PHY emulation with fixed speed/link PHYs"
 	depends on PHYLIB=y
--- a/drivers/net/phy/Makefile
+++ b/drivers/net/phy/Makefile
@@ -20,6 +20,7 @@ obj-$(CONFIG_ADM6996_PHY)	+= adm6996.o
 obj-$(CONFIG_MVSWITCH_PHY)	+= mvswitch.o
 obj-$(CONFIG_IP17XX_PHY)	+= ip17xx.o
 obj-$(CONFIG_REALTEK_PHY)	+= realtek.o
+obj-$(CONFIG_AR8216_PHY)	+= ar8216.o
 obj-$(CONFIG_LSI_ET1011C_PHY)	+= et1011c.o
 obj-$(CONFIG_FIXED_PHY)		+= fixed.o
 obj-$(CONFIG_MDIO_BITBANG)	+= mdio-bitbang.o
