From c93c2bbf0cc96da5a47d77f01daf6c983cfe4216 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Tue, 29 May 2012 10:52:25 +0200
Subject: [PATCH] MIPS: BCM63XX: add 96328avng reference board

---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |   77 +++++++++++++++++++++++++++++
 1 files changed, 77 insertions(+), 0 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -54,6 +54,80 @@
 static struct board_info board;
 
 /*
+ * known 6328 boards
+ */
+#ifdef CONFIG_BCM63XX_CPU_6328
+static struct board_info __initdata board_96328avng = {
+	.name				= "96328avng",
+	.expected_cpu_id		= 0x6328,
+
+	.has_uart0			= 1,
+	.has_pci			= 1,
+
+	.has_enetsw			= 1,
+
+	.enetsw = {
+		.used_ports = {
+			[0] = {
+				.used	= 1,
+				.phy_id = 1,
+				.name	= "Port 1",
+			},
+			[1] = {
+				.used	= 1,
+				.phy_id	= 2,
+				.name	= "Port 2",
+			},
+			[2] = {
+				.used	= 1,
+				.phy_id	= 3,
+				.name	= "Port 3",
+			},
+			[3] = {
+				.used	= 1,
+				.phy_id	= 4,
+				.name	= "Port 4",
+			},
+		},
+	},
+
+	.leds = {
+		{
+			.name		= "96328avng::internet-fail",
+			.gpio		= 2,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96328avng::dsl",
+			.gpio		= 3,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96328avng::power",
+			.gpio		= 4,
+			.active_low	= 1,
+			.default_trigger = "default-on",
+		},
+		{
+			.name		= "96328avng::power-fail",
+			.gpio		= 8,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96328avng::wps",
+			.gpio		= 9,
+			.active_low	= 1,
+		},
+		{
+			.name		= "96328avng::internet",
+			.gpio		= 11,
+			.active_low	= 1,
+		},
+	},
+};
+#endif
+
+/*
  * known 6338 boards
  */
 #ifdef CONFIG_BCM63XX_CPU_6338
@@ -2246,6 +2320,9 @@ static struct board_info __initdata boar
  * all boards
  */
 static const struct board_info __initdata *bcm963xx_boards[] = {
+#ifdef CONFIG_BCM63XX_CPU_6328
+	&board_96328avng,
+#endif
 #ifdef CONFIG_BCM63XX_CPU_6338
 	&board_96338gw,
 	&board_96338w,
