#!/bin/sh
#
# Copyright (C) 2012 OpenWrt.org
#

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

. /lib/functions/uci-defaults.sh
. /lib/brcm63xx.sh

ucidef_set_interface_loopback

case "$board_name" in

96328avng |\
963281TAN |\
96348A-122 |\
96358-502V |\
CT6373-1 |\
AW4339U |\
CPVA642 |\
CT536_CT5621 |\
D-4P-W |\
NB6 |\
SPW303V |\
SPW500V |\
V2110 |\
96348W3)
	ucidef_set_interface_lan "eth0"
	;;

AW4139)
	ucidef_set_interface_lan "eth0.1"
	ucidef_add_switch "eth0" "1" "1"
	ucidef_add_switch_vlan "eth0" "1" "0 1 2 3 4 5t"
	;;

DVG3810BN)
	ucidef_set_interfaces_lan_wan "eth1.1" "eth0"
	ucidef_add_switch "eth1" "1" "1"
	ucidef_add_switch_vlan "eth1" "1" "0 1 2 3 4 5t"
	;;

*)
	ucidef_set_interfaces_lan_wan "eth1" "eth0"
	;;

esac

uci commit network

exit 0
