--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -393,6 +393,16 @@ config USB_CNS3XXX_OHCI
 	  Enable support for the CNS3XXX SOC's on-chip OHCI controller.
 	  It is needed for low-speed USB 1.0 device support.
 
+config USB_OHCI_HCD_PLATFORM
+	bool "Generic OHCI driver for a platform device"
+	depends on USB_OHCI_HCD && EXPERIMENTAL
+	default n
+	---help---
+	  Adds an OHCI host driver for a generic platform device, which
+	  provieds a memory space and an irq.
+
+	  If unsure, say N.
+
 config USB_OHCI_BIG_ENDIAN_DESC
 	bool
 	depends on USB_OHCI_HCD
--- a/drivers/usb/host/ohci-hcd.c
+++ b/drivers/usb/host/ohci-hcd.c
@@ -1121,6 +1121,11 @@ MODULE_LICENSE ("GPL");
 #define PLATFORM_DRIVER		ohci_xls_driver
 #endif
 
+#ifdef CONFIG_USB_OHCI_HCD_PLATFORM
+#include "ohci-platform.c"
+#define PLATFORM_DRIVER		ohci_platform_driver
+#endif
+
 #if	!defined(PCI_DRIVER) &&		\
 	!defined(PLATFORM_DRIVER) &&	\
 	!defined(OMAP1_PLATFORM_DRIVER) &&	\
--- /dev/null
+++ b/drivers/usb/host/ohci-platform.c
@@ -0,0 +1,194 @@
+/*
+ * Generic platform ohci driver
+ *
+ * Copyright 2007 Michael Buesch <m@bues.ch>
+ * Copyright 2011-2012 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Derived from the OCHI-SSB driver
+ * Derived from the OHCI-PCI driver
+ * Copyright 1999 Roman Weissgaerber
+ * Copyright 2000-2002 David Brownell
+ * Copyright 1999 Linus Torvalds
+ * Copyright 1999 Gregory P. Smith
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+#include <linux/platform_device.h>
+#include <linux/usb/ohci_pdriver.h>
+
+static int ohci_platform_reset(struct usb_hcd *hcd)
+{
+	struct platform_device *pdev = to_platform_device(hcd->self.controller);
+	struct usb_ohci_pdata *pdata = pdev->dev.platform_data;
+	struct ohci_hcd *ohci = hcd_to_ohci(hcd);
+	int err;
+
+	if (pdata->big_endian_desc)
+		ohci->flags |= OHCI_QUIRK_BE_DESC;
+	if (pdata->big_endian_mmio)
+		ohci->flags |= OHCI_QUIRK_BE_MMIO;
+	if (pdata->no_big_frame_no)
+		ohci->flags |= OHCI_QUIRK_FRAME_NO;
+
+	ohci_hcd_init(ohci);
+	err = ohci_init(ohci);
+
+	return err;
+}
+
+static int ohci_platform_start(struct usb_hcd *hcd)
+{
+	struct ohci_hcd *ohci = hcd_to_ohci(hcd);
+	int err;
+
+	err = ohci_run(ohci);
+	if (err < 0) {
+		ohci_err(ohci, "can't start\n");
+		ohci_stop(hcd);
+	}
+
+	return err;
+}
+
+static const struct hc_driver ohci_platform_hc_driver = {
+	.description		= hcd_name,
+	.product_desc		= "Generic Platform OHCI Controller",
+	.hcd_priv_size		= sizeof(struct ohci_hcd),
+
+	.irq			= ohci_irq,
+	.flags			= HCD_MEMORY | HCD_USB11,
+
+	.reset			= ohci_platform_reset,
+	.start			= ohci_platform_start,
+	.stop			= ohci_stop,
+	.shutdown		= ohci_shutdown,
+
+	.urb_enqueue		= ohci_urb_enqueue,
+	.urb_dequeue		= ohci_urb_dequeue,
+	.endpoint_disable	= ohci_endpoint_disable,
+
+	.get_frame_number	= ohci_get_frame,
+
+	.hub_status_data	= ohci_hub_status_data,
+	.hub_control		= ohci_hub_control,
+#ifdef	CONFIG_PM
+	.bus_suspend		= ohci_bus_suspend,
+	.bus_resume		= ohci_bus_resume,
+#endif
+
+	.start_port_reset	= ohci_start_port_reset,
+};
+
+static int __devinit ohci_platform_probe(struct platform_device *dev)
+{
+	struct usb_hcd *hcd;
+	struct resource *res_mem;
+	int irq;
+	int err = -ENOMEM;
+
+	BUG_ON(!dev->dev.platform_data);
+
+	if (usb_disabled())
+		return -ENODEV;
+
+	irq = platform_get_irq(dev, 0);
+	if (irq < 0) {
+		pr_err("no irq provieded");
+		return irq;
+	}
+
+	res_mem = platform_get_resource(dev, IORESOURCE_MEM, 0);
+	if (!res_mem) {
+		pr_err("no memory recourse provieded");
+		return -ENXIO;
+	}
+
+	hcd = usb_create_hcd(&ohci_platform_hc_driver, &dev->dev,
+			dev_name(&dev->dev));
+	if (!hcd)
+		return -ENOMEM;
+
+	hcd->rsrc_start = res_mem->start;
+	hcd->rsrc_len = resource_size(res_mem);
+
+	if (!request_mem_region(hcd->rsrc_start, hcd->rsrc_len, hcd_name)) {
+		pr_err("controller already in use");
+		err = -EBUSY;
+		goto err_put_hcd;
+	}
+
+	hcd->regs = ioremap_nocache(hcd->rsrc_start, hcd->rsrc_len);
+	if (!hcd->regs)
+		goto err_release_region;
+	err = usb_add_hcd(hcd, irq, IRQF_SHARED);
+	if (err)
+		goto err_iounmap;
+
+	platform_set_drvdata(dev, hcd);
+
+	return err;
+
+err_iounmap:
+	iounmap(hcd->regs);
+err_release_region:
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+err_put_hcd:
+	usb_put_hcd(hcd);
+	return err;
+}
+
+static int __devexit ohci_platform_remove(struct platform_device *dev)
+{
+	struct usb_hcd *hcd = platform_get_drvdata(dev);
+
+	usb_remove_hcd(hcd);
+	iounmap(hcd->regs);
+	release_mem_region(hcd->rsrc_start, hcd->rsrc_len);
+	usb_put_hcd(hcd);
+	platform_set_drvdata(dev, NULL);
+
+	return 0;
+}
+
+#ifdef CONFIG_PM
+
+static int ohci_platform_suspend(struct device *dev)
+{
+	return 0;
+}
+
+static int ohci_platform_resume(struct device *dev)
+{
+	struct usb_hcd *hcd = dev_get_drvdata(dev);
+
+	ohci_finish_controller_resume(hcd);
+	return 0;
+}
+
+#else /* !CONFIG_PM */
+#define ohci_platform_suspend	NULL
+#define ohci_platform_resume	NULL
+#endif /* CONFIG_PM */
+
+static const struct platform_device_id ohci_platform_table[] = {
+	{ "ohci-platform", 0 },
+	{ }
+};
+MODULE_DEVICE_TABLE(platform, ohci_platform_table);
+
+static const struct dev_pm_ops ohci_platform_pm_ops = {
+	.suspend	= ohci_platform_suspend,
+	.resume		= ohci_platform_resume,
+};
+
+static struct platform_driver ohci_platform_driver = {
+	.id_table	= ohci_platform_table,
+	.probe		= ohci_platform_probe,
+	.remove		= __devexit_p(ohci_platform_remove),
+	.shutdown	= usb_hcd_platform_shutdown,
+	.driver		= {
+		.owner	= THIS_MODULE,
+		.name	= "ohci-platform",
+		.pm	= &ohci_platform_pm_ops,
+	}
+};
--- /dev/null
+++ b/include/linux/usb/ohci_pdriver.h
@@ -0,0 +1,38 @@
+/*
+ * Copyright (C) 2012 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * This program is free software; you can redistribute it and/or modify it
+ * under the terms of the GNU General Public License as published by the
+ * Free Software Foundation; either version 2 of the License, or (at your
+ * option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful, but
+ * WITHOUT ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
+ * or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License
+ * for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software Foundation,
+ * Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#ifndef __USB_CORE_OHCI_PDRIVER_H
+#define __USB_CORE_OHCI_PDRIVER_H
+
+/**
+ * struct usb_ohci_pdata - platform_data for generic ohci driver
+ *
+ * @big_endian_desc:	BE descriptors
+ * @big_endian_mmio:	BE registers
+ * @no_big_frame_no:	no big endian frame_no shift
+ *
+ * These are general configuration options for the OHCI controller. All of
+ * these options are activating more or less workarounds for some hardware.
+ */
+struct usb_ohci_pdata {
+	unsigned	big_endian_desc:1;
+	unsigned	big_endian_mmio:1;
+	unsigned	no_big_frame_no:1;
+};
+
+#endif /* __USB_CORE_OHCI_PDRIVER_H */
