From 658afad639a9456e1bb6fe5bba0032f3c0c3f699 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Tue, 1 May 2012 14:10:39 +0200
Subject: [PATCH 62/79] MTD: bcm63xxpart: use nvram for PSI size

---
 drivers/mtd/bcm63xxpart.c |    4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

--- a/drivers/mtd/bcm63xxpart.c
+++ b/drivers/mtd/bcm63xxpart.c
@@ -32,6 +32,7 @@
 #include <linux/mtd/mtd.h>
 #include <linux/mtd/partitions.h>
 
+#include <asm/mach-bcm63xx/bcm63xx_nvram.h>
 #include <asm/mach-bcm63xx/bcm963xx_tag.h>
 #include <asm/mach-bcm63xx/board_bcm963xx.h>
 
@@ -90,7 +91,8 @@ static int bcm63xx_parse_cfe_partitions(
 			      BCM63XX_CFE_BLOCK_SIZE);
 
 	cfelen = cfe_erasesize;
-	nvramlen = cfe_erasesize;
+	nvramlen = bcm63xx_nvram_get_psi_size() * 1024;
+	nvramlen = roundup(nvramlen, cfe_erasesize);
 
 	/* Allocate memory for buffer */
 	buf = vmalloc(sizeof(struct bcm_tag));
