--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -227,6 +227,12 @@ config LEDS_BD2802
 	  This option enables support for BD2802GU RGB LED driver chips
 	  accessed via the I2C bus.
 
+config LEDS_GTA02_VIBRATOR
+	boolean "Vibrator Support for the Openmoko Freerunner GSM phone"
+	depends on LEDS_CLASS && MACH_NEO1973_GTA02
+ 	help
+	  This option enables support for the vibrator on the Openmoko Freerunner.
+
 comment "LED Triggers"
 
 config LEDS_TRIGGERS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -30,6 +30,7 @@ obj-$(CONFIG_LEDS_PWM)			+= leds-pwm.o
 
 # LED SPI Drivers
 obj-$(CONFIG_LEDS_DAC124S085)		+= leds-dac124s085.o
+obj-$(CONFIG_LEDS_GTA02_VIBRATOR)	+= leds-gta02-vibrator.o
 
 # LED Triggers
 obj-$(CONFIG_LEDS_TRIGGER_TIMER)	+= ledtrig-timer.o
