--- a/arch/mips/ath79/dev-wmac.c
+++ b/arch/mips/ath79/dev-wmac.c
@@ -15,6 +15,7 @@
 #include <linux/init.h>
 #include <linux/delay.h>
 #include <linux/irq.h>
+#include <linux/etherdevice.h>
 #include <linux/platform_device.h>
 #include <linux/ath9k_platform.h>
 
@@ -22,6 +23,7 @@
 #include <asm/mach-ath79/ar71xx_regs.h>
 #include "dev-wmac.h"
 
+static u8 ath79_wmac_mac[ETH_ALEN];
 static struct ath9k_platform_data ath79_wmac_data;
 
 static struct resource ath79_wmac_resources[] = {
@@ -134,7 +136,7 @@ static void qca955x_wmac_setup(void)
 		ath79_wmac_data.is_clk_25mhz = true;
 }
 
-void __init ath79_register_wmac(u8 *cal_data)
+void __init ath79_register_wmac(u8 *cal_data, u8 *mac_addr)
 {
 	if (soc_is_ar913x())
 		ar913x_wmac_setup();
@@ -151,5 +153,10 @@ void __init ath79_register_wmac(u8 *cal_
 		memcpy(ath79_wmac_data.eeprom_data, cal_data,
 		       sizeof(ath79_wmac_data.eeprom_data));
 
+	if (mac_addr) {
+		memcpy(ath79_wmac_mac, mac_addr, sizeof(ath79_wmac_mac));
+		ath79_wmac_data.macaddr = ath79_wmac_mac;
+	}
+
 	platform_device_register(&ath79_wmac_device);
 }
--- a/arch/mips/ath79/dev-wmac.h
+++ b/arch/mips/ath79/dev-wmac.h
@@ -12,6 +12,6 @@
 #ifndef _ATH79_DEV_WMAC_H
 #define _ATH79_DEV_WMAC_H
 
-void ath79_register_wmac(u8 *cal_data);
+void ath79_register_wmac(u8 *cal_data, u8 *mac_addr);
 
 #endif /* _ATH79_DEV_WMAC_H */
--- a/arch/mips/ath79/mach-ap81.c
+++ b/arch/mips/ath79/mach-ap81.c
@@ -98,7 +98,7 @@ static void __init ap81_setup(void)
 					ap81_gpio_keys);
 	ath79_register_spi(&ap81_spi_data, ap81_spi_info,
 			   ARRAY_SIZE(ap81_spi_info));
-	ath79_register_wmac(cal_data);
+	ath79_register_wmac(cal_data, NULL);
 	ath79_register_usb();
 }
 
--- a/arch/mips/ath79/mach-db120.c
+++ b/arch/mips/ath79/mach-db120.c
@@ -134,7 +134,7 @@ static void __init db120_setup(void)
 	ath79_register_spi(&db120_spi_data, db120_spi_info,
 			   ARRAY_SIZE(db120_spi_info));
 	ath79_register_usb();
-	ath79_register_wmac(art + DB120_WMAC_CALDATA_OFFSET);
+	ath79_register_wmac(art + DB120_WMAC_CALDATA_OFFSET, NULL);
 	db120_pci_init(art + DB120_PCIE_CALDATA_OFFSET);
 }
 
--- a/arch/mips/ath79/mach-ap121.c
+++ b/arch/mips/ath79/mach-ap121.c
@@ -91,7 +91,7 @@ static void __init ap121_setup(void)
 	ath79_register_spi(&ap121_spi_data, ap121_spi_info,
 			   ARRAY_SIZE(ap121_spi_info));
 	ath79_register_usb();
-	ath79_register_wmac(cal_data);
+	ath79_register_wmac(cal_data, NULL);
 }
 
 MIPS_MACHINE(ATH79_MACH_AP121, "AP121", "Atheros AP121 reference board",
