--- a/arch/arm/mach-gemini/board-wbd222.c
+++ b/arch/arm/mach-gemini/board-wbd222.c
@@ -151,6 +151,7 @@ static void __init wbd222_init(void)
 	platform_register_watchdog();
 	platform_device_register(&wbd222_phy_device);
 	platform_register_ethernet(&gmac_data);
+	platform_register_usb(0);
 }
 
 MACHINE_START(WBD222, "Wiliboard WBD-222")
