--- a/arch/mips/Kconfig
+++ b/arch/mips/Kconfig
@@ -92,11 +92,13 @@ config ATH79
 
 config BCM47XX
 	bool "Broadcom BCM47XX based boards"
+	select BOOT_RAW
 	select CEVT_R4K
 	select CSRC_R4K
 	select DMA_NONCOHERENT
 	select HW_HAS_PCI
 	select IRQ_CPU
+	select NO_EXCEPT_FILL
 	select SYS_SUPPORTS_32BIT_KERNEL
 	select SYS_SUPPORTS_LITTLE_ENDIAN
 	select GENERIC_GPIO
