From 635d5a2ac8aa483c3a0635c60bff8ea8978ff6a7 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Sun, 11 Dec 2011 18:34:13 +0100
Subject: [PATCH 39/47] MIPS: ath79: add USB platform setup code for AR934X

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 arch/mips/ath79/dev-usb.c                      |   28 ++++++++++++++++++++++++
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |    7 ++++++
 2 files changed, 35 insertions(+), 0 deletions(-)

--- a/arch/mips/ath79/dev-usb.c
+++ b/arch/mips/ath79/dev-usb.c
@@ -193,6 +193,32 @@ static void __init ar933x_usb_setup(void
 	platform_device_register(&ath79_ehci_device);
 }
 
+static void __init ar934x_usb_setup(void)
+{
+	u32 bootstrap;
+
+	bootstrap = ath79_reset_rr(AR934X_RESET_REG_BOOTSTRAP);
+	if (bootstrap & AR934X_BOOTSTRAP_USB_MODE_DEVICE)
+		return;
+
+	ath79_device_reset_set(AR934X_RESET_USBSUS_OVERRIDE);
+	udelay(1000);
+
+	ath79_device_reset_clear(AR934X_RESET_USB_PHY);
+	udelay(1000);
+
+	ath79_device_reset_clear(AR934X_RESET_USB_PHY_ANALOG);
+	udelay(1000);
+
+	ath79_device_reset_clear(AR934X_RESET_USB_HOST);
+	udelay(1000);
+
+	ath79_usb_init_resource(ath79_ehci_resources, AR934X_EHCI_BASE,
+				AR934X_EHCI_SIZE, ATH79_CPU_IRQ_USB);
+	ath79_ehci_device.dev.platform_data = &ath79_ehci_pdata_v2;
+	platform_device_register(&ath79_ehci_device);
+}
+
 void __init ath79_register_usb(void)
 {
 	if (soc_is_ar71xx())
@@ -205,6 +231,8 @@ void __init ath79_register_usb(void)
 		ar913x_usb_setup();
 	else if (soc_is_ar933x())
 		ar933x_usb_setup();
+	else if (soc_is_ar934x())
+		ar934x_usb_setup();
 	else
 		BUG();
 }
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -63,6 +63,8 @@
 
 #define AR934X_WMAC_BASE	(AR71XX_APB_BASE + 0x00100000)
 #define AR934X_WMAC_SIZE	0x20000
+#define AR934X_EHCI_BASE	0x1b000000
+#define AR934X_EHCI_SIZE	0x200
 
 /*
  * DDR_CTRL block
@@ -288,6 +290,11 @@
 #define AR933X_RESET_USB_PHY		BIT(4)
 #define AR933X_RESET_USBSUS_OVERRIDE	BIT(3)
 
+#define AR934X_RESET_USB_PHY_ANALOG	BIT(11)
+#define AR934X_RESET_USB_HOST		BIT(5)
+#define AR934X_RESET_USB_PHY		BIT(4)
+#define AR934X_RESET_USBSUS_OVERRIDE	BIT(3)
+
 #define AR933X_BOOTSTRAP_REF_CLK_40	BIT(0)
 
 #define AR934X_BOOTSTRAP_SW_OPTION8	BIT(23)
