From c7c3c338cb25d7f55ddb3f6bfbf3572758ca3896 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Thu, 10 Nov 2011 16:53:08 +0100
Subject: [PATCH 50/79] MTD: DEVICES: m25p80: use parsers if provided in flash
 platform data

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 drivers/mtd/devices/m25p80.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/mtd/devices/m25p80.c
+++ b/drivers/mtd/devices/m25p80.c
@@ -986,7 +986,8 @@ static int __devinit m25p_probe(struct s
 	/* partitions should match sector boundaries; and it may be good to
 	 * use readonly partitions for writeprotected sectors (BP2..BP0).
 	 */
-	return mtd_device_parse_register(&flash->mtd, NULL, &ppdata,
+	return mtd_device_parse_register(&flash->mtd,
+			data ? data->part_probe_types : NULL, &ppdata,
 			data ? data->parts : NULL,
 			data ? data->nr_parts : 0);
 }
