--- a/drivers/leds/Kconfig
+++ b/drivers/leds/Kconfig
@@ -498,4 +498,12 @@ config LEDS_TRIGGER_USBDEV
 	  This allows LEDs to be controlled by the presence/activity of
 	  an USB device. If unsure, say N.
 
+config LEDS_TRIGGER_ADM5120_SWITCH
+	tristate "LED ADM5120 Switch Port Status Trigger"
+	depends on LEDS_TRIGGERS && ADM5120
+	help
+	  This allows LEDs to be controlled by the port states of
+	  the ADM5120 built-in Ethernet Switch
+	  If unsure, say N.
+
 endif # NEW_LEDS
--- a/drivers/leds/Makefile
+++ b/drivers/leds/Makefile
@@ -60,3 +60,4 @@ obj-$(CONFIG_LEDS_TRIGGER_DEFAULT_ON)	+=
 obj-$(CONFIG_LEDS_TRIGGER_MORSE)	+= ledtrig-morse.o
 obj-$(CONFIG_LEDS_TRIGGER_NETDEV)	+= ledtrig-netdev.o
 obj-$(CONFIG_LEDS_TRIGGER_USBDEV)	+= ledtrig-usbdev.o
+obj-$(CONFIG_LEDS_TRIGGER_ADM5120_SWITCH) += ledtrig-adm5120-switch.o
