--- a/drivers/input/misc/Kconfig
+++ b/drivers/input/misc/Kconfig
@@ -220,6 +220,15 @@ config HP_SDC_RTC
 	  Say Y here if you want to support the built-in real time clock
 	  of the HP SDC controller.
 
+config INPUT_LIS302DL
+	tristate "STmicro LIS302DL 3-axis accelerometer"
+	depends on SPI_MASTER
+	help
+	  SPI driver for the STmicro LIS302DL 3-axis accelerometer.
+
+	  The userspece interface is a 3-axis (X/Y/Z) relative movement
+	  Linux input device, reporting REL_[XYZ] events.
+
 config INPUT_PCF50633_PMU
 	tristate "PCF50633 PMU events"
 	depends on MFD_PCF50633
--- a/drivers/input/misc/Makefile
+++ b/drivers/input/misc/Makefile
@@ -25,3 +25,4 @@ obj-$(CONFIG_INPUT_UINPUT)		+= uinput.o
 obj-$(CONFIG_INPUT_WISTRON_BTNS)	+= wistron_btns.o
 obj-$(CONFIG_INPUT_YEALINK)		+= yealink.o
 obj-$(CONFIG_INPUT_GPIO_BUTTONS)	+= gpio_buttons.o
+obj-$(CONFIG_INPUT_LIS302DL)		+= lis302dl.o
