
--- a/drivers/usb/host/Kconfig
+++ b/drivers/usb/host/Kconfig
@@ -645,3 +645,15 @@ config USB_HCD_BCMA
 	  for ehci and ohci.
 
 	  If unsure, say N.
+
+config USB_HCD_SSB
+	tristate "SSB usb host driver"
+	depends on SSB && EXPERIMENTAL
+	select USB_OHCI_HCD_PLATFORM if USB_OHCI_HCD
+	select USB_EHCI_HCD_PLATFORM if USB_EHCI_HCD
+	help
+	  Enbale support for the EHCI and OCHI host controller on an bcma bus.
+	  It converts the bcma driver into two platform device drivers
+	  for ehci and ohci.
+
+	  If unsure, say N.
--- a/drivers/usb/host/Makefile
+++ b/drivers/usb/host/Makefile
@@ -38,3 +38,4 @@ obj-$(CONFIG_USB_FSL_MPH_DR_OF)	+= fsl-m
 obj-$(CONFIG_USB_OCTEON2_COMMON) += octeon2-common.o
 obj-$(CONFIG_MIPS_ALCHEMY)	+= alchemy-common.o
 obj-$(CONFIG_USB_HCD_BCMA)	+= bcma-hcd.o
+obj-$(CONFIG_USB_HCD_SSB)	+= ssb-hcd.o
--- /dev/null
+++ b/drivers/usb/host/ssb-hcd.c
@@ -0,0 +1,279 @@
+/*
+ * Sonics Silicon Backplane
+ * Broadcom USB-core driver  (SSB bus glue)
+ *
+ * Copyright 2011-2012 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Based on ssb-ohci driver
+ * Copyright 2007 Michael Buesch <m@bues.ch>
+ *
+ * Derived from the OHCI-PCI driver
+ * Copyright 1999 Roman Weissgaerber
+ * Copyright 2000-2002 David Brownell
+ * Copyright 1999 Linus Torvalds
+ * Copyright 1999 Gregory P. Smith
+ *
+ * Derived from the USBcore related parts of Broadcom-SB
+ * Copyright 2005-2011 Broadcom Corporation
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+#include <linux/ssb/ssb.h>
+#include <linux/delay.h>
+#include <linux/platform_device.h>
+#include <linux/module.h>
+#include <linux/usb/ehci_pdriver.h>
+#include <linux/usb/ohci_pdriver.h>
+
+MODULE_AUTHOR("Hauke Mehrtens");
+MODULE_DESCRIPTION("Common USB driver for SSB Bus");
+MODULE_LICENSE("GPL");
+
+#define SSB_HCD_TMSLOW_HOSTMODE	(1 << 29)
+
+struct ssb_hcd_device {
+	struct platform_device *ehci_dev;
+	struct platform_device *ohci_dev;
+
+	u32 enable_flags;
+};
+
+static void __devinit ssb_hcd_5354wa(struct ssb_device *dev)
+{
+#ifdef CONFIG_SSB_DRIVER_MIPS
+	/* Work around for 5354 failures */
+	if (dev->id.revision == 2 && dev->bus->chip_id == 0x5354) {
+		/* Change syn01 reg */
+		ssb_write32(dev, 0x894, 0x00fe00fe);
+
+		/* Change syn03 reg */
+		ssb_write32(dev, 0x89c, ssb_read32(dev, 0x89c) | 0x1);
+	}
+#endif
+}
+
+static void __devinit ssb_hcd_usb20wa(struct ssb_device *dev)
+{
+	if (dev->id.coreid == SSB_DEV_USB20_HOST) {
+		/*
+		 * USB 2.0 special considerations:
+		 *
+		 * In addition to the standard SSB reset sequence, the Host
+		 * Control Register must be programmed to bring the USB core
+		 * and various phy components out of reset.
+		 */
+		ssb_write32(dev, 0x200, 0x7ff);
+
+		/* Change Flush control reg */
+		ssb_write32(dev, 0x400, ssb_read32(dev, 0x400) & ~8);
+		ssb_read32(dev, 0x400);
+
+		/* Change Shim control reg */
+		ssb_write32(dev, 0x304, ssb_read32(dev, 0x304) & ~0x100);
+		ssb_read32(dev, 0x304);
+
+		udelay(1);
+
+		ssb_hcd_5354wa(dev);
+	}
+}
+
+/* based on arch/mips/brcm-boards/bcm947xx/pcibios.c */
+static u32 __devinit ssb_hcd_init_chip(struct ssb_device *dev)
+{
+	u32 flags = 0;
+
+	if (dev->id.coreid == SSB_DEV_USB11_HOSTDEV)
+		/* Put the device into host-mode. */
+		flags |= SSB_HCD_TMSLOW_HOSTMODE;
+
+	ssb_device_enable(dev, flags);
+
+	ssb_hcd_usb20wa(dev);
+
+	return flags;
+}
+
+static const struct usb_ehci_pdata ehci_pdata = {
+};
+
+static const struct usb_ohci_pdata ohci_pdata = {
+};
+
+static struct platform_device * __devinit
+ssb_hcd_create_pdev(struct ssb_device *dev, bool ohci, u32 addr, u32 len)
+{
+	struct platform_device *hci_dev;
+	struct resource hci_res[2];
+	int ret = -ENOMEM;
+
+	memset(hci_res, 0, sizeof(hci_res));
+
+	hci_res[0].start = addr;
+	hci_res[0].end = hci_res[0].start + len - 1;
+	hci_res[0].flags = IORESOURCE_MEM;
+
+	hci_res[1].start = dev->irq;
+	hci_res[1].flags = IORESOURCE_IRQ;
+
+	hci_dev = platform_device_alloc(ohci ? "ohci-platform" :
+					"ehci-platform" , 0);
+	if (!hci_dev)
+		return NULL;
+
+	hci_dev->dev.parent = dev->dev;
+	hci_dev->dev.dma_mask = &hci_dev->dev.coherent_dma_mask;
+
+	ret = platform_device_add_resources(hci_dev, hci_res,
+					    ARRAY_SIZE(hci_res));
+	if (ret)
+		goto err_alloc;
+	if (ohci)
+		ret = platform_device_add_data(hci_dev, &ohci_pdata,
+					       sizeof(ohci_pdata));
+	else
+		ret = platform_device_add_data(hci_dev, &ehci_pdata,
+					       sizeof(ehci_pdata));
+	if (ret)
+		goto err_alloc;
+	ret = platform_device_add(hci_dev);
+	if (ret)
+		goto err_alloc;
+
+	return hci_dev;
+
+err_alloc:
+	platform_device_put(hci_dev);
+	return ERR_PTR(ret);
+}
+
+static int __devinit ssb_hcd_probe(struct ssb_device *dev,
+				   const struct ssb_device_id *id)
+{
+	int err, tmp;
+	int start, len;
+	u16 chipid_top;
+	u16 coreid = dev->id.coreid;
+	struct ssb_hcd_device *usb_dev;
+
+	/* USBcores are only connected on embedded devices. */
+	chipid_top = (dev->bus->chip_id & 0xFF00);
+	if (chipid_top != 0x4700 && chipid_top != 0x5300)
+		return -ENODEV;
+
+	/* TODO: Probably need checks here; is the core connected? */
+
+	if (dma_set_mask(dev->dma_dev, DMA_BIT_MASK(32)) ||
+	    dma_set_coherent_mask(dev->dma_dev, DMA_BIT_MASK(32)))
+		return -EOPNOTSUPP;
+
+	usb_dev = kzalloc(sizeof(struct ssb_hcd_device), GFP_KERNEL);
+	if (!usb_dev)
+		return -ENOMEM;
+
+	/* We currently always attach SSB_DEV_USB11_HOSTDEV
+	 * as HOST OHCI. If we want to attach it as Client device,
+	 * we must branch here and call into the (yet to
+	 * be written) Client mode driver. Same for remove(). */
+	usb_dev->enable_flags = ssb_hcd_init_chip(dev);
+
+	tmp = ssb_read32(dev, SSB_ADMATCH0);
+
+	start = ssb_admatch_base(tmp);
+	len = (coreid == SSB_DEV_USB20_HOST) ? 0x800 : ssb_admatch_size(tmp);
+	usb_dev->ohci_dev = ssb_hcd_create_pdev(dev, true, start, len);
+	if (IS_ERR(usb_dev->ohci_dev)) {
+		err = PTR_ERR(usb_dev->ohci_dev);
+		goto err_free_usb_dev;
+	}
+
+	if (coreid == SSB_DEV_USB20_HOST) {
+		start = ssb_admatch_base(tmp) + 0x800; /* ehci core offset */
+		usb_dev->ehci_dev = ssb_hcd_create_pdev(dev, false, start, len);
+		if (IS_ERR(usb_dev->ehci_dev)) {
+			err = PTR_ERR(usb_dev->ehci_dev);
+			goto err_unregister_ohci_dev;
+		}
+	}
+
+	ssb_set_drvdata(dev, usb_dev);
+	return 0;
+
+err_unregister_ohci_dev:
+	platform_device_unregister(usb_dev->ohci_dev);
+err_free_usb_dev:
+	kfree(usb_dev);
+	return err;
+}
+
+static void __devexit ssb_hcd_remove(struct ssb_device *dev)
+{
+	struct ssb_hcd_device *usb_dev = ssb_get_drvdata(dev);
+	struct platform_device *ohci_dev = usb_dev->ohci_dev;
+	struct platform_device *ehci_dev = usb_dev->ehci_dev;
+
+	if (ohci_dev)
+		platform_device_unregister(ohci_dev);
+	if (ehci_dev)
+		platform_device_unregister(ehci_dev);
+
+	ssb_device_disable(dev, 0);
+}
+
+static void __devexit ssb_hcd_shutdown(struct ssb_device *dev)
+{
+	ssb_device_disable(dev, 0);
+}
+
+#ifdef CONFIG_PM
+
+static int ssb_hcd_suspend(struct ssb_device *dev, pm_message_t state)
+{
+	ssb_device_disable(dev, 0);
+
+	return 0;
+}
+
+static int ssb_hcd_resume(struct ssb_device *dev)
+{
+	struct ssb_hcd_device *usb_dev = ssb_get_drvdata(dev);
+
+	ssb_device_enable(dev, usb_dev->enable_flags);
+
+	return 0;
+}
+
+#else /* !CONFIG_PM */
+#define ssb_hcd_suspend	NULL
+#define ssb_hcd_resume	NULL
+#endif /* CONFIG_PM */
+
+static const struct ssb_device_id ssb_hcd_table[] __devinitconst = {
+	SSB_DEVICE(SSB_VENDOR_BROADCOM, SSB_DEV_USB11_HOSTDEV, SSB_ANY_REV),
+	SSB_DEVICE(SSB_VENDOR_BROADCOM, SSB_DEV_USB11_HOST, SSB_ANY_REV),
+	SSB_DEVICE(SSB_VENDOR_BROADCOM, SSB_DEV_USB20_HOST, SSB_ANY_REV),
+	SSB_DEVTABLE_END
+};
+MODULE_DEVICE_TABLE(ssb, ssb_hcd_table);
+
+static struct ssb_driver ssb_hcd_driver = {
+	.name		= KBUILD_MODNAME,
+	.id_table	= ssb_hcd_table,
+	.probe		= ssb_hcd_probe,
+	.remove		= __devexit_p(ssb_hcd_remove),
+	.shutdown	= ssb_hcd_shutdown,
+	.suspend	= ssb_hcd_suspend,
+	.resume		= ssb_hcd_resume,
+};
+
+static int __init ssb_hcd_init(void)
+{
+	return ssb_driver_register(&ssb_hcd_driver);
+}
+module_init(ssb_hcd_init);
+
+static void __exit ssb_hcd_exit(void)
+{
+	ssb_driver_unregister(&ssb_hcd_driver);
+}
+module_exit(ssb_hcd_exit);
