Arduino - Byte

Arduino

Guide

Tutorials

Reference

Hardware

Software

Forum

Playground

Exhibition

Hacking

FAQ

Buy

Language | Libraries | Comparison

## byte

#### Description

Bytes store an 8-bit number, from 0 to 255.

#### Example

        byte b = B10010;  // "B" is the binary formatter (18 decimal)

#### See also

- int
- unsigned int
- long
- unsigned long
- integer constants

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

Edit Page | Page History | Printable View | Recent Site Changes