Arduino - Max

Arduino

Guide

Tutorials

Reference

Hardware

Software

Forum

Playground

Exhibition

Hacking

FAQ

Buy

Language | Libraries | Comparison

## max(x, y)

#### Description

Calculates the maximum of two numbers.

#### Parameters

x: the first number, any data type

y: the second number, any data type

#### Returns

The larger of the two numbers.

#### Example

    sensVal = max(senVal, 20); // assigns sensVal to the bigger of sensVal or 20 (effectively ensuring that it is at least 20)

#### See also

- min()
- constrain()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

Edit Page | Page History | Printable View | Recent Site Changes