Arduino - Byte

Arduino

Buy | Download | Getting Started | Learning | Reference | Hardware | FAQ

Blog » | Forum » | Playground »

Reference Language (extended) | Libraries | Comparison | Board

## byte

#### Description

Bytes store an 8-bit number, from 0 to 255. byte is an unsigned data type, meaning that it does not store negative numbers.

#### Example

        byte b = B10010;  // "B" is the binary formatter (18 decimal)

#### See also

- int
- unsigned int
- long
- unsigned long
- integer constants

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | All Recent Site Changes