##############################################################

Generation_Series.name=Gen6 & Gen6 Deluxe 
Generation_Series.upload.protocol=stk500
Generation_Series.upload.maximum_size=63488
Generation_Series.upload.speed=38400
Generation_Series.bootloader.low_fuses=0xFF
Generation_Series.bootloader.high_fuses=0xDC
Generation_Series.bootloader.extended_fuses=0xFD
Generation_Series.bootloader.path=atmega644p
Generation_Series.bootloader.file=ATmegaBOOT_644P.hex
Generation_Series.bootloader.unlock_bits=0x3F
Generation_Series.bootloader.lock_bits=0x0F
Generation_Series.build.mcu=atmega644p
Generation_Series.build.f_cpu=16000000L
Generation_Series.build.core=arduino


##############################################################


Sanguinololu.name=Sanguinololu 1.2 and above
Sanguinololu.upload.protocol=stk500
Sanguinololu.upload.maximum_size=63488
Sanguinololu.upload.speed=38400
Sanguinololu.bootloader.low_fuses=0xFF
Sanguinololu.bootloader.high_fuses=0xDC
Sanguinololu.bootloader.extended_fuses=0xFD
Sanguinololu.bootloader.path=atmega644p
Sanguinololu.bootloader.file=ATmegaBOOT_644P.hex
Sanguinololu.bootloader.unlock_bits=0x3F
Sanguinololu.bootloader.lock_bits=0x0F
Sanguinololu.build.mcu=atmega644p
Sanguinololu.build.f_cpu=16000000L
Sanguinololu.build.core=arduino
