Python: module skeinforge_application.skeinforge_plugins.craft_plugins.unpause

skeinforge_application.skeinforge_plugins.craft_plugins.unpause ($Date: 2008/21/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/fabmetheus/skeinforge_application/skeinforge_plugins/craft_plugins/unpause.py

Previous / Next / Contents

`
The unpause plugin is based on the Shane Hathaway's patch to speed up a line segment to compensate for the delay of the microprocessor. The description is at:
http://shane.willowrise.com/archives/delay-compensation-in-firmware/
The unpause manual page is at:
http://fabmetheus.crsndoo.com/wiki/index.php/Skeinforge_Unpause
Operation
Settings
Delay
Maximum Speed
Examples
`

## Operation

The default 'Activate Unpause' checkbox is off. When it is on, the functions described below will work, when it is off, nothing will be done.

## Settings

### Delay

Default is 28 milliseconds, which Shane found for the Arduino.
Defines the delay on the microprocessor that will be at least partially compensated for.

### Maximum Speed

Default is 1.3.
Defines the maximum amount that the feed rate will be sped up to, compared to the original feed rate.

## Examples

The following examples unpause the file Screw Holder Bottom.stl. The examples are run in a terminal in the folder which contains Screw Holder Bottom.stl and unpause.py.
> python unpause.py
This brings up the unpause dialog.
> python unpause.py Screw Holder Bottom.stl
The unpause tool is parsing the file:
Screw Holder Bottom.stl
..
The unpause tool has created the file:
.. Screw Holder Bottom_unpause.gcode

Previous / Next / Contents

Modules

``

__init__ fabmetheus_utilities.archive fabmetheus_utilities.euclidean | fabmetheus_utilities.fabmetheus_tools.fabmetheus_interpret fabmetheus_utilities.gcodec fabmetheus_utilities.intercircle | math fabmetheus_utilities.settings skeinforge_application.skeinforge_utilities.skeinforge_craft | skeinforge_application.skeinforge_utilities.skeinforge_polyfile skeinforge_application.skeinforge_utilities.skeinforge_profile sys

Classes

``

UnpauseRepository
UnpauseSkein

class UnpauseRepository
`` | `A class to handle the unpause settings. `

Methods defined here:

__init__(self)
  `Set the default settings, execute title & settings fileName.`

execute(self)
  `Unpause button has been clicked.`

class UnpauseSkein
`` | `A class to unpause a skein of extrusions. `

Methods defined here:

__init__(self)

getCraftedGcode(self, gcodeText, repository)
  `Parse gcode text and store the unpause gcode.`

getUnpausedArcMovement(self, line, splitLine)
  `Get an unpaused arc movement.`

getUnpausedLinearMovement(self, line, splitLine)
  `Get an unpaused linear movement.`

getUnpausedMovement(self, distance, line, splitLine)
  `Get an unpaused movement.`

parseInitialization(self)
  `Parse gcode initialization and store the parameters.`

parseLine(self, line)
  `Parse a gcode line.`

Functions

``

getCraftedText(fileName, gcodeText, repository=None)
  `Unpause a gcode linear move file or text.`

getCraftedTextFromText(gcodeText, repository=None)
  `Unpause a gcode linear move text.`

getNewRepository()
  `Get new repository.`

getSelectedPlugin(repository)
  `Get the selected plugin.`

main()
  `Display the unpause dialog.`

writeOutput(fileName, shouldAnalyze=True)
  `Unpause a gcode linear move file.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __date__ = '$Date: 2008/21/04 $' __license__ = 'GNU Affero General Public License http://www.gnu.org/licenses/agpl.html' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)