From 8fd28bca39e31be5a05cb9cf89335a207e8b031f Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 3 Aug 2012 09:53:54 +0200
Subject: [PATCH 08/25] spi support

---
 drivers/spi/Kconfig  |   17 +++++++++++++++++
 drivers/spi/Makefile |    3 +++
 2 files changed, 20 insertions(+), 0 deletions(-)

diff --git a/drivers/spi/Kconfig b/drivers/spi/Kconfig
index f62424f..7e8146e 100644
--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -188,6 +188,10 @@ config SPI_MPC52xx
 	  This drivers supports the MPC52xx SPI controller in master SPI
 	  mode.
 
+config SPI_FALCON
+	tristate "Falcon SPI controller support"
+	depends on SOC_FALCON
+
 config SPI_MPC52xx_PSC
 	tristate "Freescale MPC52xx PSC SPI controller"
 	depends on PPC_MPC52xx && EXPERIMENTAL
@@ -362,6 +366,11 @@ config SPI_TOPCLIFF_PCH
 	  This driver also supports the ML7213/ML7223/ML7831, a companion chip
 	  for the Atom E6xx series and compatible with the Intel EG20T PCH.
 
+config SPI_SVIP
+	tristate "SVIP SPI controller"
+	depends on SOC_SVIP
+	default y
+
 config SPI_TXX9
 	tristate "Toshiba TXx9 SPI controller"
 	depends on GENERIC_GPIO && CPU_TX49XX
@@ -387,6 +396,14 @@ config SPI_NUC900
 	help
 	  SPI driver for Nuvoton NUC900 series ARM SoCs
 
+config SPI_XWAY
+	tristate "Lantiq XWAY SPI controller"
+	depends on LANTIQ && SOC_TYPE_XWAY
+	select SPI_BITBANG
+	help
+	  This driver supports the Lantiq SoC SPI controller in master
+	  mode.
+
 #
 # Add new SPI master controllers in alphabetical order above this line
 #
diff --git a/drivers/spi/Makefile b/drivers/spi/Makefile
index 1514c1d..71e7655 100644
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -25,6 +25,7 @@ obj-$(CONFIG_SPI_DW_MMIO)		+= spi-dw-mmio.o
 obj-$(CONFIG_SPI_DW_PCI)		+= spi-dw-midpci.o
 spi-dw-midpci-objs			:= spi-dw-pci.o spi-dw-mid.o
 obj-$(CONFIG_SPI_EP93XX)		+= spi-ep93xx.o
+obj-$(CONFIG_SPI_FALCON)		+= spi-falcon.o
 obj-$(CONFIG_SPI_FSL_LIB)		+= spi-fsl-lib.o
 obj-$(CONFIG_SPI_FSL_ESPI)		+= spi-fsl-espi.o
 obj-$(CONFIG_SPI_FSL_SPI)		+= spi-fsl-spi.o
@@ -59,4 +60,6 @@ obj-$(CONFIG_SPI_TLE62X0)		+= spi-tle62x0.o
 obj-$(CONFIG_SPI_TOPCLIFF_PCH)		+= spi-topcliff-pch.o
 obj-$(CONFIG_SPI_TXX9)			+= spi-txx9.o
 obj-$(CONFIG_SPI_XILINX)		+= spi-xilinx.o
+obj-$(CONFIG_SPI_XWAY)			+= spi-xway.o
+obj-$(CONFIG_SPI_SVIP)			+= spi_svip.o
 
-- 
1.7.9.1

