--- a/drivers/mtd/Kconfig
+++ b/drivers/mtd/Kconfig
@@ -158,7 +158,7 @@ config MTD_BCM63XX_PARTS
 
 config MTD_WRT160NL_PARTS
 	tristate "Linksys WRT160NL partitioning support"
-	depends on MTD_PARTITIONS && ATH79_MACH_WRT160NL
+	depends on ATH79_MACH_WRT160NL
 	---help---
 	   Linksys WRT160NL partitioning support
 
@@ -178,6 +178,12 @@ config MTD_MYLOADER_PARTS
 	  You will still need the parsing functions to be called by the driver
 	  for your particular device. It won't happen automatically.
 
+config MTD_TPLINK_PARTS
+	tristate "TP-Link AR7XXX/AR9XXX partitioning support"
+	depends on ATH79
+	---help---
+	  TBD.
+
 comment "User Modules And Translation Layers"
 
 config MTD_CHAR
--- a/drivers/mtd/Makefile
+++ b/drivers/mtd/Makefile
@@ -13,6 +13,7 @@ obj-$(CONFIG_MTD_AFS_PARTS)	+= afs.o
 obj-$(CONFIG_MTD_AR7_PARTS)	+= ar7part.o
 obj-$(CONFIG_MTD_BCM63XX_PARTS)	+= bcm63xxpart.o
 obj-$(CONFIG_MTD_MYLOADER_PARTS) += myloader.o
+obj-$(CONFIG_MTD_TPLINK_PARTS)	+= tplinkpart.o
 obj-$(CONFIG_MTD_WRT160NL_PARTS) += wrt160nl_part.o
 
 # 'Users' - code which presents functionality to userspace.
