From 6824bc23dfaf2ff75cc6c6e9281e12ceb45fe1b3 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 3 Aug 2012 10:30:01 +0200
Subject: [PATCH 24/25] fritzbox ram

---
 arch/mips/lantiq/setup.c |    6 ++++++
 1 files changed, 6 insertions(+), 0 deletions(-)

diff --git a/arch/mips/lantiq/setup.c b/arch/mips/lantiq/setup.c
index 708e969..114989d 100644
--- a/arch/mips/lantiq/setup.c
+++ b/arch/mips/lantiq/setup.c
@@ -40,6 +40,12 @@ void __init plat_mem_setup(void)
 			e += 8;
 			if (strict_strtoul(e, 0, &memsize))
 				pr_warn("bad memsize specified\n");
+		} else if (!strcmp(e, "memsize")) {
+			envp++;
+			e = (char *)KSEG1ADDR(*envp);
+			if (strict_strtoul(e, 0, &memsize))
+				pr_warn("bad memsize specified\n");
+			memsize /= 1024 * 1024;
 		}
 		if (!strncmp(e, "BRN-BOOT", 8)){
 			pr_info("Found BRN-BOOT instead of u-boot\n");
-- 
1.7.9.1

