From 5a39e76b3ea2f7dbf04f7dd2210536068583eaf6 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Fri, 3 Aug 2012 09:54:22 +0200
Subject: [PATCH 11/25] i2c support

---
 drivers/i2c/busses/Kconfig  |   10 ++++++++++
 drivers/i2c/busses/Makefile |    1 +
 2 files changed, 11 insertions(+), 0 deletions(-)

diff --git a/drivers/i2c/busses/Kconfig b/drivers/i2c/busses/Kconfig
index 3101dd5..e8d149d 100644
--- a/drivers/i2c/busses/Kconfig
+++ b/drivers/i2c/busses/Kconfig
@@ -369,6 +369,16 @@ config I2C_DESIGNWARE_PCI
 	  This driver can also be built as a module.  If so, the module
 	  will be called i2c-designware-pci.
 
+config I2C_FALCON
+	tristate "Falcon I2C interface"
+	depends on SOC_FALCON
+	help
+	  If you say yes to this option, support will be included for the
+	  Lantiq FALC-ON I2C core.
+
+	  This driver can also be built as a module. If so, the module
+	  will be called i2c-falcon.
+
 config I2C_GPIO
 	tristate "GPIO-based bitbanging I2C"
 	depends on GENERIC_GPIO
diff --git a/drivers/i2c/busses/Makefile b/drivers/i2c/busses/Makefile
index fba6da6..36239c8 100644
--- a/drivers/i2c/busses/Makefile
+++ b/drivers/i2c/busses/Makefile
@@ -37,6 +37,7 @@ obj-$(CONFIG_I2C_DESIGNWARE_PLATFORM)	+= i2c-designware-platform.o
 i2c-designware-platform-objs := i2c-designware-platdrv.o i2c-designware-core.o
 obj-$(CONFIG_I2C_DESIGNWARE_PCI)	+= i2c-designware-pci.o
 i2c-designware-pci-objs := i2c-designware-pcidrv.o i2c-designware-core.o
+obj-$(CONFIG_I2C_FALCON)	+= i2c-falcon.o
 obj-$(CONFIG_I2C_GPIO)		+= i2c-gpio.o
 obj-$(CONFIG_I2C_HIGHLANDER)	+= i2c-highlander.o
 obj-$(CONFIG_I2C_IBM_IIC)	+= i2c-ibm_iic.o
-- 
1.7.9.1

