Index: avr.c
===================================================================
--- gcc/config/avr/avr.c	(Revision 144406)
+++ gcc/config/avr/avr.c	(Arbeitskopie)
@@ -76,6 +76,12 @@ static rtx avr_function_value (const_tre
 static void avr_insert_attributes (tree, tree *);
 static void avr_asm_init_sections (void);
 static unsigned int avr_section_type_flags (tree, const char *, int);
+static void avr_asm_named_section (const char *name, unsigned int flags, tree decl);
+/* Track if code will use .bss and/or .data */
+static int avr_need_clear_bss_p = 0;
+static int avr_need_copy_data_p = 0;
+static void avr_output_data_section_asm_op (const void*);
+static void avr_output_bss_section_asm_op (const void*);
 
 static void avr_reorg (void);
 static void avr_asm_out_ctor (rtx, int);
@@ -4886,6 +4892,54 @@ avr_output_progmem_section_asm_op (const
   fprintf (asm_out_file, "\t.p2align 1\n");
 }
 
+/* ASM_OUTPUT_COMMON */
+/* Track need of __do_clear_bss */
+
+void
+avr_asm_output_common (FILE *stream, const char *name,
+                       unsigned HOST_WIDE_INT size,
+                       unsigned HOST_WIDE_INT rounded ATTRIBUTE_UNUSED)
+{
+    avr_need_clear_bss_p = 1;
+    fputs ("\t.comm ", stream);
+    assemble_name (stream, name);
+    fprintf (stream, ",%lu,1\n", (unsigned long) size);  
+}
+
+/* ASM_OUTPUT_LOCAL */
+/* Track need of __do_clear_bss */
+
+void
+avr_asm_output_local (FILE *stream, const char *name,
+                      unsigned HOST_WIDE_INT size,
+                      unsigned HOST_WIDE_INT rounded ATTRIBUTE_UNUSED)
+{                                                    
+    avr_need_clear_bss_p = 1;                           
+    fputs ("\t.lcomm ", stream);                      
+    assemble_name (stream, name);                   
+    fprintf (stream, ",%d\n", (int) size);           
+}
+
+/* Unnamed section callback to track need of __do_copy_data */
+
+static void
+avr_output_data_section_asm_op (const void *data)
+{
+    avr_need_copy_data_p = 1;
+    /* Dispatch to default */
+    output_section_asm_op (data);
+}
+
+/* Unnamed section callback to track need of __do_clear_bss */
+
+static void
+avr_output_bss_section_asm_op (const void *data)
+{
+    avr_need_clear_bss_p = 1;
+    /* Dispatch to default */
+    output_section_asm_op (data);
+}
+
 /* Implement TARGET_ASM_INIT_SECTIONS.  */
 
 static void
@@ -4895,6 +4949,27 @@ avr_asm_init_sections (void)
 					 avr_output_progmem_section_asm_op,
 					 NULL);
   readonly_data_section = data_section;
+
+  data_section->unnamed.callback = avr_output_data_section_asm_op;
+  bss_section->unnamed.callback = avr_output_bss_section_asm_op;
+}
+
+/* TARGET_ASM_NAMED_SECTION */
+/* Track need of __do_clear_bss, __do_copy_data for named sections */
+
+static void
+avr_asm_named_section (const char *name, unsigned int flags, tree decl)
+{
+    if (!avr_need_copy_data_p)
+        avr_need_copy_data_p =
+            (0 == strncmp (name, ".data", 5)
+             || 0 == strncmp (name, ".rodata", 7)
+             || 0 == strncmp (name, ".gnu.linkonce.", 14));
+    
+    if (!avr_need_clear_bss_p)
+        avr_need_clear_bss_p = (0 == strncmp (name, ".bss", 4));
+    
+    default_elf_asm_named_section (name, flags, decl);
 }
 
 static unsigned int
@@ -4933,12 +5008,6 @@ avr_file_start (void)
   
   fputs ("__tmp_reg__ = 0\n" 
          "__zero_reg__ = 1\n", asm_out_file);
-
-  /* FIXME: output these only if there is anything in the .data / .bss
-     sections - some code size could be saved by not linking in the
-     initialization code from libgcc if one or both sections are empty.  */
-  fputs ("\t.global __do_copy_data\n", asm_out_file);
-  fputs ("\t.global __do_clear_bss\n", asm_out_file);
 }
 
 /* Outputs to the stdio stream FILE some
@@ -4947,6 +5016,16 @@ avr_file_start (void)
 static void
 avr_file_end (void)
 {
+    /* Output these only if there is anything in the
+       .data* / .rodata* / .gnu.linkonce.* resp. .bss*
+       input section(s) - some code size can be saved by not
+       linking in the initialization code from libgcc if resp.
+       sections are empty. */
+    if (avr_need_copy_data_p)
+        fputs (".global __do_copy_data\n", asm_out_file);
+    
+    if (avr_need_clear_bss_p)
+        fputs (".global __do_clear_bss\n", asm_out_file);
 }
 
 /* Choose the order in which to allocate hard registers for
Index: avr.h
===================================================================
--- gcc/config/avr/avr.h	(Revision 144406)
+++ gcc/config/avr/avr.h	(Arbeitskopie)
@@ -544,29 +544,21 @@ do {									    \
 #define ASM_APP_OFF "/* #NOAPP */\n"
 
 /* Switch into a generic section.  */
-#define TARGET_ASM_NAMED_SECTION default_elf_asm_named_section
+#define TARGET_ASM_NAMED_SECTION avr_asm_named_section
 #define TARGET_ASM_INIT_SECTIONS avr_asm_init_sections
 
 #define ASM_OUTPUT_ASCII(FILE, P, SIZE)	 gas_output_ascii (FILE,P,SIZE)
 
 #define IS_ASM_LOGICAL_LINE_SEPARATOR(C, STR) ((C) == '\n' || ((C) == '$'))
 
-#define ASM_OUTPUT_COMMON(STREAM, NAME, SIZE, ROUNDED)			   \
-do {									   \
-     fputs ("\t.comm ", (STREAM));					   \
-     assemble_name ((STREAM), (NAME));					   \
-     fprintf ((STREAM), ",%lu,1\n", (unsigned long)(SIZE));		   \
-} while (0)
+#define ASM_OUTPUT_COMMON(STREAM, NAME, SIZE, ROUNDED) \
+        avr_asm_output_common (STREAM, NAME, SIZE, ROUNDED)
 
-#define ASM_OUTPUT_BSS(FILE, DECL, NAME, SIZE, ROUNDED)			\
-  asm_output_bss ((FILE), (DECL), (NAME), (SIZE), (ROUNDED))
+#define ASM_OUTPUT_BSS(FILE, DECL, NAME, SIZE, ROUNDED) \
+        asm_output_bss ((FILE), (DECL), (NAME), (SIZE), (ROUNDED))
 
-#define ASM_OUTPUT_LOCAL(STREAM, NAME, SIZE, ROUNDED)			\
-do {									\
-     fputs ("\t.lcomm ", (STREAM));					\
-     assemble_name ((STREAM), (NAME));					\
-     fprintf ((STREAM), ",%d\n", (int)(SIZE));				\
-} while (0)
+#define ASM_OUTPUT_LOCAL(STREAM, NAME, SIZE, ROUNDED) \
+        avr_asm_output_local (STREAM, NAME, SIZE, ROUNDED)
 
 #undef TYPE_ASM_OP
 #undef SIZE_ASM_OP
--- gcc/config/avr/avr-protos.h.orig	2009-03-13 08:12:25.962726300 -0600
+++ gcc/config/avr/avr-protos.h	2009-03-13 09:08:46.027900400 -0600
@@ -38,6 +38,8 @@ extern int avr_simple_epilogue (void);
 extern void gas_output_limited_string (FILE *file, const char *str);
 extern void gas_output_ascii (FILE *file, const char *str, size_t length);
 extern int avr_hard_regno_rename_ok (unsigned int, unsigned int);
+extern void avr_asm_output_common (FILE *stream, const char *name, unsigned HOST_WIDE_INT size, unsigned HOST_WIDE_INT rounded);
+extern void avr_asm_output_local (FILE *stream, const char *name, unsigned HOST_WIDE_INT size, unsigned HOST_WIDE_INT rounded);
 
 #ifdef TREE_CODE
 extern void asm_output_external (FILE *file, tree decl, char *name);
@@ -124,6 +126,7 @@ extern RTX_CODE avr_normalize_condition 
 extern int compare_eq_p (rtx insn);
 extern void out_shift_with_cnt (const char *template, rtx insn,
 				rtx operands[], int *len, int t_len);
+extern rtx avr_return_addr_rtx (int count, rtx tem);
 extern int avr_io_address_p (rtx x, int size);
 extern int avr_peep2_scratch_safe (rtx reg_rtx);
 #endif /* RTX_CODE */
